{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":34,"n_cols":17,"rows_kept":34,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FHA-A / RZQG-L(8)Y1"]
[]
[]
[]
[]
["","","","","FHA35AVEB / FHA35AVEB / FHA35AVEB / FHA35AVEB / RZQG125L8Y1B","FHA35AVEB / FHA35AVEB / FHA35AVEB / RZQG100L8Y1B","FHA50AVEB / FHA50AVEB / FHA50AVEB / RZQG125L8Y1B","FHA50AVEB / FHA50AVEB / RZQG100L8Y1B","FHA60AVEB / FHA60AVEB / RZQG125L8Y1B","FHA50AVEB / FHA50AVEB / RZQG71L8Y1B","FHA71AVEB / RZQG71L8Y1B","FHA35AVEB / FHA35AVEB / RZQG71L8Y1B","FHA35AVEB / FHA35AVEB / FHA35AVEB / RZQG71L8Y1B","FHA71AVEB / FHA71AVEB / RZQG100L8Y1B","FHA50AVEB / FHA50AVEB / FHA50AVEB / RZQG100L8Y1B","FHA35AVEB / FHA35AVEB / FHA35AVEB / FHA35AVEB / RZQG100L8Y1B","FHA71AVEB / FHA71AVEB / RZQG125L8Y1B"]
["Wydajność chłodnicza","Nom.","","kW","","","","","","","6.80 (1)"]
["Chłodzenie pomieszczeń","SEER","","","","","","","","5.10","6.86","5.10","5.10","5.10","5.10","5.10"]
["","Roczne zużycie energii","","kWh/rok","","","","","","467","347","467","467","652","652","652"]
["","Wydajność","Pdesign","kW","","","","","","6.80","6.80","6.80","6.80","9.50","9.50","9.50"]
["","Klasa efektywności energetycznej","","","","","","","","A","A++","A","A","A","A","A"]
["Ogrzewanie pomieszczeń (przeciętny klimat)","Wydajność","Pdesign","kW","","","","","","6.00","7.60","6.00","6.00","11.30","11.30","11.30"]
["","SCOP/A","","","","","","","","3.80","4.32","3.80","3.80","3.80","3.80","3.80"]
["","Klasa efektywności energetycznej","","","","","","","","A","A+","A","A","A","A","A"]
["","Roczne zużycie energii","","kWh/rok","","","","","","2,211","2,463","2,211","2,211","4,164","4,164","4,164"]
["Efektywność nominalna","Annual energy consumption","","kWh","","","","","","","890"]
["","EER","","","","","","","","","3.82 (3)"]
["","COP","","","","","","","","","4.13 (3)"]
["","Dyrektywa na temat oznaczeń zużycia energii (klas energetycznych)","Chłodzenie","","","","","","","","A"]
["","","Ogrzewanie","","","","","","","","A"]
["Wydajność grzewcza","Nom.","","kW","","","","","","","7.50 (2)"]
["Zakres efektywności energetycznej","","","","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","","","","","","","","A+++ ~ D"]
["Uwagi","","","","","","","","","","(1) - Chłodzenie: temp. wewn. 27°CDB, 19,0°CWB; temp. zewn. 35°CDB; długość równoważna instalacji rurowej: 7,5m; różnica poziomów: 0 m","(1) - Chłodzenie: temp. wewn. 27°CDB, 19,0°CWB; temp. zewn. 35°CDB; długość równoważna instalacji rurowej: 7,5m; różnica poziomów: 0 m"]
["","","","","","","","","","","(2) - Grzanie: temp. wewn. 20°CDB; temp. zewnętrzna 7°CDB, 6°CWB , równoważna instalacja chłodnicza: 7,5 m; różnica poziomów: 0 m","(2) - Grzanie: temp. wewn. 20°CDB; temp. zewnętrzna 7°CDB, 6°CWB , równoważna instalacja chłodnicza: 7,5 m; różnica poziomów: 0 m"]
["","","","","","","","","","","(3) - Wartości EER/COP według Eurovent 2012, do użytkowania tylko poza Unią Europejską","(3) - Wartości EER/COP według Eurovent 2012, do użytkowania tylko poza Unią Europejską"]
["Chłodzenie pomieszczeń","Klasa efektywności energetycznej","","","","","","","","","","","","","","","A"]
["","Wydajność","Pdesign","kW","","","","","","","","","","","","","12.00"]
["","SEER","","","","","","","","","","","","","","","5.10"]
["","Roczne zużycie energii","","kWh/rok","","","","","","","","","","","","","824"]
["Ogrzewanie pomieszczeń (przeciętny klimat)","Klasa efektywności energetycznej","","","","","","","","","","","","","","","A"]
["","Wydajność","Pdesign","kW","","","","","","","","","","","","","12.71"]
["","SCOP/A","","","","","","","","","","","","","","","3.80"]
["","Pdh Wydajność grzewcza w temp. -10°","","kW","","","","","","","","","","","","","11"]
["","Roczne zużycie energii","","kWh/rok","","","","","","","","","","","","","4683"]