{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":18,"n_cols":11,"rows_kept":18,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FHA-A / RZQSG-L3/9V1"]
[]
[]
[]
[]
["","","","","FHA71AVEB / RZQSG71L3V1B","FHA50AVEB / FHA50AVEB / FHA50AVEB / RZQSG125L9V1B","FHA50AVEB / FHA50AVEB / RZQSG100L9V1B","FHA60AVEB / FHA60AVEB / RZQSG125L9V1B","FHA35AVEB / FHA35AVEB / RZQSG71L3V1B","FHA35AVEB / FHA35AVEB / FHA35AVEB / RZQSG100L9V1B","FHA35AVEB / FHA35AVEB / FHA35AVEB / FHA35AVEB / RZQSG125L9V1B"]
["Chłodzenie pomieszczeń","Roczne zużycie energii","","kWh/rok","","","","","467","652","875"]
["","Wydajność","Pdesign","kW","","","","","6.80","9.50","12.0"]
["Ogrzewanie pomieszczeń (przeciętny klimat)","Wydajność","Pdesign","kW","","","","","6.00","7.60","7.60"]
["","Roczne zużycie energii","","kWh/rok","","","","","2,211","2,800","2,800"]
["Zakres efektywności energetycznej","","","","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D"]
["Chłodzenie pomieszczeń","SEER","","","","","","","5.10","5.10","4.80"]
["","Klasa efektywności energetycznej","","","","","","","A","A","B"]
["Ogrzewanie pomieszczeń (przeciętny klimat)","SCOP/A","","","","","","","3.80","3.80","3.80"]
["","Klasa efektywności energetycznej","","","","","","","A","A","A"]
["Uwagi","","","","","","","","(1) - Chłodzenie: temp. wewn. 27°CDB, 19,0°CWB; temp. zewn. 35°CDB; długość równoważna instalacji rurowej: 7,5m; różnica poziomów: 0 m","(1) - Chłodzenie: temp. wewn. 27°CDB, 19,0°CWB; temp. zewn. 35°CDB; długość równoważna instalacji rurowej: 7,5m; różnica poziomów: 0 m","(1) - Chłodzenie: temp. wewn. 27°CDB, 19,0°CWB; temp. zewn. 35°CDB; długość równoważna instalacji rurowej: 7,5m; różnica poziomów: 0 m"]
["","","","","","","","","(2) - Grzanie: temp. wewn. 20°CDB; temp. zewnętrzna 7°CDB, 6°CWB , równoważna instalacja chłodnicza: 7,5 m; różnica poziomów: 0 m","(2) - Grzanie: temp. wewn. 20°CDB; temp. zewnętrzna 7°CDB, 6°CWB , równoważna instalacja chłodnicza: 7,5 m; różnica poziomów: 0 m","(2) - Grzanie: temp. wewn. 20°CDB; temp. zewnętrzna 7°CDB, 6°CWB , równoważna instalacja chłodnicza: 7,5 m; różnica poziomów: 0 m"]
["","","","","","","","","(3) - Wartości EER/COP według Eurovent 2012, do użytkowania tylko poza Unią Europejską","(3) - Wartości EER/COP według Eurovent 2012, do użytkowania tylko poza Unią Europejską","(3) - Wartości EER/COP według Eurovent 2012, do użytkowania tylko poza Unią Europejską"]