{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":38,"n_cols":8,"rows_kept":38,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FHA-A"]
[]
[]
[]
[]
["","","","","FHA35AVEB","FHA50AVEB","FHA60AVEB","FHA71AVEB"]
["Poziom ciśnienia akustycznego","Grzanie","Wysoki","dBA","36","37","37","38"]
["","","Nom.","dBA","34","35","35","36"]
["","","Czynnik","dBA","31","32","33","34"]
["","Chłodzenie","Czynnik","dBA","34","35","35","36"]
["","","Niski","dBA","31","32","33","34"]
["","","Wysoki","dBA","36","37","37","38"]
["Standardowe akcesoria","Rura izolacji cieplnej","","","2","2","2","2"]
["","Materiał obejmy przewodów elektrycznych","","","7","7","7","7"]
["","Opaska zaciskowa przewodu elastycznego","","","1","1","1","1"]
["","Przewód spustowy","","","1","1","1","1"]
["","Podkładka","","","8","8","8","8"]
["","Podkładka uszczelniająca (duża)","","","1","1","1","1"]
["","Podkładka uszczelniająca (mała)","","","1","1","1","1"]
["","przepust z materiału żywicznego","","","1","1","1","1"]
["","Śruby","","","2","2","2","2"]
["","uchwyt okablowania","","","2","2","2","2"]
["Syst. kontroli","Wired remote control","","","BRC1E53A7, BRC1E53B7, BRC1E53C7, BRC1D528, BRC1E51A7","BRC1E53A7, BRC1E53B7, BRC1E53C7, BRC1D528, BRC1E51A7","BRC1E53A7, BRC1E53B7, BRC1E53C7, BRC1D528, BRC1E51A7","BRC1E53A7, BRC1E53B7, BRC1E53C7, BRC1D528, BRC1E51A7"]
["","Infrared remote control","","","BRC7GA53, BRC7GA56","BRC7GA53, BRC7GA56","BRC7GA53, BRC7GA56","BRC7GA53, BRC7GA56"]
["Połączenia instalacji rurowej","Ciecz","Śr. zewn.","mm","6.35","6.35","6.35","9.52"]
["","Gaz","Śr. zewn.","mm","9.50","12.7","12.7","15.9"]
["","Spust","","","VP20","VP20","VP20","VP20"]
["Poziom mocy akustycznej","Chłodzenie","","dBA","53","54","54","55"]
["Wymiary","Jednostka","Szerokość","mm","960","960","1,270","1,270"]
["","","Głębokość","mm","690","690","690","690"]
["","","Wysokość","mm","235","235","235","235"]
["Obudowa","Materiał","","","żywica, blacha cienka","żywica, blacha cienka","żywica, blacha cienka","żywica, blacha cienka"]
["","Kolor","","","Biały","Biały","Biały","Biały"]
["Ciężar","Jednostka","","kg","24.0","25.0","31.0","32.0"]
["Power supply","liczba faz","","","1~","1~","1~","1~"]
["","Częstotliwość","","Hz","50","50","50","50"]
["","Napięcie","","V","220-240","220-240","220-240","220-240"]
["Uwagi","","","","(1) - Dane elektryczne, patrz oddzielny rysunek","(1) - Dane elektryczne, patrz oddzielny rysunek","(1) - Dane elektryczne, patrz oddzielny rysunek","(1) - Dane elektryczne, patrz oddzielny rysunek"]