{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":24,"n_cols":12,"rows_kept":24,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FHQ-C / RZQSG-L(8)Y1"]
[]
[]
[]
[]
["","","","","FHQ100CAVEB / RZQSG100L8Y1B","FHQ35CAVEB / FHQ35CAVEB / FHQ35CAVEB / RZQSG100L8Y1B","FHQ50CAVEB / FHQ50CAVEB / RZQSG100L8Y1B","FHQ50CAVEB / FHQ50CAVEB / FHQ50CAVEB / RZQSG125L8Y1B","FHQ35CAVEB / FHQ35CAVEB / FHQ35CAVEB / FHQ35CAVEB / RZQSG125L8Y1B","FHQ60CAVEB / FHQ60CAVEB / RZQSG125L8Y1B","FHQ125CAVEB / RZQSG125L8Y1B","FHQ140CAVEB / RZQSG140L7Y1B"]
["Wydajność chłodnicza","Nom.","","kW","9.5","","","","","","12.0","13.4"]
["Chłodzenie pomieszczeń","SEER","","","5.61","5.1","5.1","4.8","4.8","4.8","5.61"]
["","Roczne zużycie energii","","kWh/rok","593","652","652","875","875","875","749"]
["","Wydajność","Pdesign","kW","9.5","9.5","9.5","12","12","12","12"]
["","Klasa efektywności energetycznej","","","A+","B","B","B","B","B","A+"]
["Ogrzewanie pomieszczeń (przeciętny klimat)","Wydajność","Pdesign","kW","7.6","7.6","7.6","7.6","7.6","7.6","7.6"]
["","SCOP/A","","","3.91","3.8","3.8","3.8","3.8","3.8","4.01"]
["","Klasa efektywności energetycznej","","","A","A","A","A","A","A","A+"]
["","Roczne zużycie energii","","kWh/rok","2,722","2,800","2,800","2,800","2,800","2,800","2,654"]
["Efektywność nominalna","Rocz. zużycie ener.","","kWh","1,480","","","","","","2,075","2,225"]
["","EER","","","3.21","","","","","","2.89","3.01"]
["","COP","","","3.61","","","","","","3.62","3.41"]
["","Dyrektywa na temat oznaczeń zużycia energii (klas energetycznych)","Chłodzenie","","A","","","","","","C"]
["","","Ogrzewanie","","A","","","","","","A"]
["Wydajność grzewcza","Nom.","","kW","10.8","","","","","","13.5","15.5"]
["Uwagi","","","","","(1) - Wartości EER/COP według Eurovent 2012, do użytkowania tylko poza Unią Europejską","(1) - Wartości EER/COP według Eurovent 2012, do użytkowania tylko poza Unią Europejską","(1) - Wartości EER/COP według Eurovent 2012, do użytkowania tylko poza Unią Europejską","(1) - Wartości EER/COP według Eurovent 2012, do użytkowania tylko poza Unią Europejską","(1) - Wartości EER/COP według Eurovent 2012, do użytkowania tylko poza Unią Europejską"]
["","","","","(1) - Wartości EER/COP według Eurovent 2012, do użytkowania tylko poza Unią Europejską","","","","","","(1) - Wartości EER/COP według Eurovent 2012, do użytkowania tylko poza Unią Europejską","(1) - Wartości EER/COP według Eurovent 2012, do użytkowania tylko poza Unią Europejską"]
["","","","","(2) - Wydaj. znam.: (chłodzenie przy temp. 35°/27° i obciążeniu znam., grzanie przy temp. 7°/20° i obciążeniu znam.)","","","","","","(2) - Wydaj. znam.: (chłodzenie przy temp. 35°/27° i obciążeniu znam., grzanie przy temp. 7°/20° i obciążeniu znam.)","(2) - Wydaj. znam.: (chłodzenie przy temp. 35°/27° i obciążeniu znam., grzanie przy temp. 7°/20° i obciążeniu znam.)"]