{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":44,"n_cols":5,"rows_kept":44,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FLXS-B9"]
[]
[]
[]
[]
["","","","","FLXS35BAVMB9"]
["Poziom ciśnienia akustycznego","Grzanie","Wysoki","dBA","46"]
["","","Cicha praca","dBA","30"]
["","","Niski","dBA","33"]
["","Chłodzenie","Cicha praca","dBA","29"]
["","","Niski","dBA","32"]
["","","Wysoki","dBA","38"]
["","","Nom.","dBA","36"]
["","Chłodzenie","Nom.","dBA","35"]
["Standardowe akcesoria","Instrukcja instalacji","","","1"]
["","Instrukcja obsługi","","","1"]
["","Zdalny sterownik bezprzewodowy","","","1"]
["","Baterie suche typu AAA","","","2"]
["","Uchwyt do pilota","","","1"]
["","Płyta montażowa","","","1"]
["","Rura izolacji cieplnej (rura chłodząca)","","","8"]
["","Filtr oczyszczający powietrze","","","1"]
["","Fotokatalityczny filtr eliminujący nieprzyjemne zapachy","","","1"]
["","Pokrywa boczna","","","2"]
["","Taśma wiążąca","","","4"]
["Syst. kontroli","Infrared remote control","","","ARC433B67"]
["Połączenia instalacji","Ciecz","Śr. zewn.","mm","6.35"]
["","Gaz","Śr. zewn.","mm","9.5"]
["","Spust","","","18"]
["Sound power level","Chłodzenie","","dBA","53"]
["","Ogrzewanie","","dBA","59"]
["Wymiary","Jednostka","Szerokość","mm","1,050"]
["","","Głębokość","mm","200"]
["","","Wysokość","mm","490"]
["Obudowa","Kolor","","","Migdałowo-biały"]
["Ciężar","Jednostka","","kg","16"]
["Power supply","liczba faz","","","1~"]
["","Częstotliwość","","Hz","50"]
["","Nazwa","","","VM"]
["","Napięcie","","V","220-240"]
["Uwagi","","","","(1) - 220 V"]
["","","","","(2) - 230 V"]
["","","","","(3) - 240 V"]
["","","","","(4) - Po podłączeniu do jednostki zewnętrznej w systemie multi, patrz specyfikacje podłączanej jednostki zewnętrznej multi."]