{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":92,"n_cols":10,"rows_kept":92,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXA-AW"]
[]
[]
[]
[]
["","","","","","FTXA20A2V1BW","FTXA25A2V1BW","FTXA35A2V1BW","FTXA42A2V1BW","FTXA50A2V1BW"]
["Poziom ciśnienia akustycznego","Grzanie","","Wysoki","dBA","39","40","41","","46"]
["","","","Czynnik","dBA","32","33","33","","42"]
["","","","Cicha praca","dBA","19","19","19","","24"]
["","","","Niski","dBA","25","25","25","","33"]
["","Chłodzenie","","Medium","dBA","32","33","33","","39"]
["","","","Cicha praca","dBA","19","19","19","","24"]
["","","","Niski","dBA","25","25","25","","31"]
["","","","Wysoki","dBA","39","40","41","","46"]
["Standardowe akcesoria","Instrukcja instalacji","","","","1","1","1","","1"]
["","Instrukcja obsługi","","","","1","1","1","","1"]
["","Filtr powietrza","","","","2","2","2","","2"]
["","Zdalny sterownik bezprzewodowy","","","","1","1","1","","1"]
["","Zdalny element sterujący płytą montażową","","","","1","1","1","","1"]
["","Torebka ze śrubami","","","","1","1","1","","1"]
["","Pokrywa na śruby","","","","1","1","1","","1"]
["","Baterie suche typu AAA","","","","2","2","2","","2"]
["","Ogólne zalecenia dotyczące bezpieczeństwa","","","","1","1","1","","1"]
["Czynnik chłodniczy","GWP","","","","675.0","675.0","675.0","","675.0"]
["Syst. kontroli","Wired remote control","","","","BRC073","BRC073","BRC073","","BRC073"]
["","Infrared remote control","","","","ARC466A58","ARC466A58","ARC466A58","","ARC466A58"]
["Połączenia instalacji","Ciecz","","Śr. zewn.","mm","6.35","6.35","6.35","","6.35"]
["","Gaz","","Śr. zewn.","mm","9.50","9.50","9.50","","12.70"]
["","Spust","","","","18","18","18","","18"]
["Power input","Chłodzenie","","Nom.","kW","0.020","0.022","0.023","","0.030"]
["","Grzanie","","Nom.","kW","0.020","0.020","0.022","","0.039"]
["Sound power level","Chłodzenie","","","dBA","57","57","60","","60"]
["Wymiary","Jednostka","","Szerokość","mm","798","798","798","","798"]
["","","","Głębokość","mm","189","189","189","","189"]
["","","","Wysokość","mm","295","295","295","","295"]
["Obudowa","Kolor","","","","Biały","Biały","Biały","","Biały"]
["Ciężar","Jednostka","","","kg","11.50","11.50","11.50","","11.50"]
["Wentylator","Przepływ powietrza","Grzanie","Wysoki","m³/min","10.9","11.1","11.5","","15.1"]
["","","","Medium","m³/min","8.7","9.0","9.0","","11.1"]
["","","","Niski","m³/min","6.4","6.4","6.4","","8.2"]
["","","","Cicha praca","m³/min","4.5","4.5","4.5","","5.7"]
["","","Chłodzenie","Niski","m³/min","6.1","6.1","6.1","","7.6"]
["","","","Medium","m³/min","8.2","8.6","8.6","","10.4"]
["","","","Wysoki","m³/min","11.0","11.5","11.9","","13.5"]
["","","","Cicha praca","m³/min","4.6","4.6","4.6","","5.2"]
["Power supply","liczba faz","","","","1~","1~","1~","","1~"]
["","Nazwa","","","","V1","V1","V1","","V1"]
["","Częstotliwość","","","Hz","50","50","50","","50"]
["","Napięcie","","","V","220-240","220-240","220-240","","220-240"]
["Pobór mocy","Chłodzenie","","Nom.","kW","","","","0.028"]
["","Grzanie","","Nom.","kW","","","","0.036"]
["Obudowa","Kolor","","","","","","","Biały"]
["Wymiary","Jednostka","","Wysokość","mm","","","","295"]
["","","","Szerokość","mm","","","","798"]
["","","","Głębokość","mm","","","","189"]
["Ciężar","Jednostka","","","kg","","","","11.50"]
["Wentylator","Przepływ powietrza","Chłodzenie","Wysoki","m³/min","","","","13.1"]
["","Natężenie przepływu powietrza","Chłodzenie","Czynnik","m³/min","","","","9.8"]
["","","","Niski","m³/min","","","","7.2"]
["","","","Cicha praca","m³/min","","","","4.6"]
["","","Grzanie","Wysoki","m³/min","","","","14.6"]
["","Natężenie przepływu powietrza","Ogrzewanie","Czynnik","m³/min","","","","10.5"]
["","","Grzanie","Niski","m³/min","","","","7.7"]
["","","","Cicha praca","m³/min","","","","5.2"]
["Poziom mocy akustycznej","Chłodzenie","","","dBA","","","","60"]
["Poziom ciśnienia akustycznego","Chłodzenie","","Wysoki","dBA","","","","45"]
["","","","Czynnik","dBA","","","","37"]
["","","","Niski","dBA","","","","29"]
["","","","Cicha praca","dBA","","","","21"]
["","Grzanie","","Wysoki","dBA","","","","45"]
["","Ogrzewanie","","Czynnik","dBA","","","","37"]
["","Grzanie","","Niski","dBA","","","","29"]
["","","","Cicha praca","dBA","","","","21"]
["Czynnik chłodniczy","GWP","","","","","","","675.0"]
["Połączenia instalacji rurowej","Ciecz","","Śr. zewn.","mm","","","","6.35"]
["","Gaz","","Śr. zewn.","mm","","","","12.70"]
["","Spust","","","","","","","18"]
["Syst. kontroli","Pilot na podczerwień","","","","","","","ARC466A58"]
["","Pilot przewodowy","","","","","","","BRC073"]
["Standardowe akcesoria","Installation manual","","","","","","","1"]
["","Screw cover","","","","","","","1"]
["","AAA dry-cell batteries","","","","","","","2"]
["","General safety precautions","","","","","","","1"]
["","Operation manual","","","","","","","1"]
["","Filtr powietrza","","","","","","","2"]
["","Infrared remote control","","","","","","","1"]
["","Remote controller mounting plate","","","","","","","1"]
["","Screw bag","","","","","","","1"]
["Zasilanie energią elektryczną","Nazwa","","","","","","","V1"]
["","liczba faz","","","","","","","1~"]
["Zasilanie","Częstotliwość","","","Hz","","","","50"]
["","Napięcie","","","V","","","","220-240"]