{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":29,"n_cols":6,"rows_kept":29,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXA-BS / RXA-B8"]
[]
[]
[]
[]
["","","","","FTXA42B2V1BS / RXA42B5V1B8","FTXA50B2V1BS / RXA50B5V1B8"]
["Wydajność chłodnicza","Min.","","kW","1.7","1.7"]
["","Nom.","","kW","4.2","5"]
["","Maks.","","kW","5","5.3"]
["Wydajność grzewcza","Min.","","kW","1.7","1.7"]
["","Nom.","","kW","5.4","5.8"]
["","Maks.","","kW","6","6.5"]
["Wydaj. znam.","EER","","","3.99","3.68"]
["","COP","","","4.12","4"]
["","Rocz. zużycie ener.","","kWh","526","679"]
["Efektywność nominalna","Dyrektywa na temat oznaczeń zużycia energii (klas energetycznych)","Chłodzenie","","A","A"]
["","","Ogrzewanie","","A","A"]
["Chłodzenie pomieszczeń","Klasa efektywności energetycznej","","","A++","A++"]
["","Wydajność","Pdesign","kW","4.2","5"]
["","SEER","","","7.5","7.33"]
["","Roczne zużycie energii","","kWh/rok","196","239"]
["Ogrzewanie pomieszczeń (przeciętny klimat)","Klasa efektywności energetycznej","","","A++","A++"]
["","Wydajność","Pdesign","kW","3.8","4"]
["","SCOP/A","","","4.6","4.6"]
["","Pdh Wydajność grzewcza w temp. -10°","","kW","3.04","3.19"]
["","Roczne zużycie energii","","kWh/rok","1156","1218"]
["Uwagi","","","","(1) - Nominalne wydajności chłodzenia oparte są na: temp. wewnętrzna: 27°CDB, 19°CWB, temp. zewn.: 35°CDB, równoważna dług. rur: 5 m, różnica poziomów: 0 m.","(1) - Nominalne wydajności chłodzenia oparte są na: temp. wewnętrzna: 27°CDB, 19°CWB, temp. zewn.: 35°CDB, równoważna dług. rur: 5 m, różnica poziomów: 0 m."]
["","","","","(2) - Nominalne wydajności grzewcze oparte są na: temperaturze wewnętrznej: 20°CDB; temperaturze zewnętrznej: 7°CDB, 6°CWB , równorzędnej instalacji chłodniczej: 5 m, różnicy poziomów: 0 m.","(2) - Nominalne wydajności grzewcze oparte są na: temperaturze wewnętrznej: 20°CDB; temperaturze zewnętrznej: 7°CDB, 6°CWB , równorzędnej instalacji chłodniczej: 5 m, różnicy poziomów: 0 m."]
["","","","","(3) - Patrz oddzielny rysunek zakresu pracy","(3) - Patrz oddzielny rysunek zakresu pracy"]