{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":30,"n_cols":6,"rows_kept":30,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXA-CB / RXA-B"]
[]
[]
[]
[]
["","","","","FTXA50C2V1BB / RXA50B5V1B","FTXA50C2V1BB / RXA50B2V1B"]
["Wydajność chłodnicza","Min.","","kW","1.70","1.70"]
["","Nom.","","kW","5.00","5.00"]
["","Maks.","","kW","5.30","5.30"]
["Wydajność grzewcza","Min.","","kW","1.70","1.70"]
["","Nom.","","kW","5.80","5.80"]
["","Maks.","","kW","6.50","6.50"]
["Wydaj. znam.","EER","","","3.68","3.68"]
["","COP","","","4.00","4.00"]
["","Rocz. zużycie ener.","","kWh","679","679"]
["Efektywność nominalna","Dyrektywa na temat oznaczeń zużycia energii (klas energetycznych)","Chłodzenie","","A","A"]
["","","Ogrzewanie","","A","A"]
["Chłodzenie pomieszczeń","Klasa efektywności energetycznej","","","A++","A++"]
["","Wydajność","Pdesign","kW","5.00","5.00"]
["","SEER","","","7.33","7.33"]
["","Roczne zużycie energii","","kWh/rok","239","239"]
["Ogrzewanie pomieszczeń (przeciętny klimat)","Klasa efektywności energetycznej","","","A++","A++"]
["","Wydajność","Pdesign","kW","4.00","4.00"]
["","SCOP/A","","","4.60","4.60"]
["","Pdh Wydajność grzewcza w temp. -10°","","kW","3.19","3.19"]
["","Roczne zużycie energii","","kWh/rok","1218","1218"]
["Zakres efektywności energetycznej","","","","","A+++ ~ D"]
["Uwagi","","","","","(1) - Nominalne wydajności chłodzenia oparte są na: temp. wewnętrzna: 27°CDB, 19°CWB, temp. zewn.: 35°CDB, równoważna dług. rur: 5 m, różnica poziomów: 0 m."]
["","","","","","(2) - Nominalne wydajności grzewcze oparte są na: temperaturze wewnętrznej: 20°CDB; temperaturze zewnętrznej: 7°CDB, 6°CWB , równorzędnej instalacji chłodniczej: 5 m, różnicy poziomów: 0 m."]
["","","","","","(3) - Patrz oddzielny rysunek zakresu pracy"]