{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":40,"n_cols":7,"rows_kept":40,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXA-CW / RXA-A8"]
[]
[]
[]
[]
["","","","","FTXA20C2V1BW / RXA20A5V1B8","FTXA25C2V1BW / RXA25A5V1B8","FTXA35C2V1BW / RXA35A5V1B8"]
["Wydajność chłodnicza","Min.","","kW","","1.30","1.40"]
["","Nom.","","kW","","2.50","3.40"]
["","Maks.","","kW","","3.20","4.00"]
["Wydajność grzewcza","Min.","","kW","","1.30","1.40"]
["","Nom.","","kW","","2.80","4.00"]
["","Maks.","","kW","","4.70","5.20"]
["Efektywność nominalna","Rocz. zużycie ener.","","kWh","","280","389"]
["","COP","","","","5.00","4.04"]
["","EER","","","","4.46","4.37"]
["","Dyrektywa na temat oznaczeń zużycia energii (klas energetycznych)","Chłodzenie","","","A","A"]
["","","Ogrzewanie","","","A","A"]
["Uwagi","","","","","(1) - Nominalne wydajności chłodzenia oparte są na: temperatura wewnętrzna: 27°CDB, 19°CWB, temp. zewn.: 35°CDB, równoważna dług. rur: 5 m, różnica poziomów: 0 m.","(1) - Nominalne wydajności chłodzenia oparte są na: temperatura wewnętrzna: 27°CDB, 19°CWB, temp. zewn.: 35°CDB, równoważna dług. rur: 5 m, różnica poziomów: 0 m."]
["","","","","","(2) - Nominalne wydajności grzewcze oparte są na: temperaturze wewnętrznej: 20°CDB; temperaturze zewnętrznej: 7°CDB, 6°CWB , równorzędnej instalacji chłodniczej: 5 m, różnicy poziomów: 0 m.","(2) - Nominalne wydajności grzewcze oparte są na: temperaturze wewnętrznej: 20°CDB; temperaturze zewnętrznej: 7°CDB, 6°CWB , równorzędnej instalacji chłodniczej: 5 m, różnicy poziomów: 0 m."]
["","","","","","(3) - Patrz oddzielny rysunek zakresu pracy","(3) - Patrz oddzielny rysunek zakresu pracy"]
["Wydajność chłodnicza","Min.","","kW","1.30"]
["","Nom.","","kW","2.00"]
["","Maks.","","kW","2.60"]
["Wydajność grzewcza","Min.","","kW","1.30"]
["","Nom.","","kW","2.50"]
["","Maks.","","kW","3.50"]
["Wydaj. znam.","EER","","","4.70"]
["","COP","","","5.00"]
["","Rocz. zużycie ener.","","kWh","213"]
["Efektywność nominalna","Dyrektywa na temat oznaczeń zużycia energii (klas energetycznych)","Chłodzenie","","A"]
["","","Ogrzewanie","","A"]
["Chłodzenie pomieszczeń","Klasa efektywności energetycznej","","","A+++"]
["","Wydajność","Pdesign","kW","2.00"]
["","SEER","","","8.75"]
["","Roczne zużycie energii","","kWh/rok","80"]
["Ogrzewanie pomieszczeń (przeciętny klimat)","Klasa efektywności energetycznej","","","A+++"]
["","Wydajność","Pdesign","kW","2.40"]
["","SCOP/A","","","5.15"]
["","Pdh Wydajność grzewcza w temp. -10°","","kW","2.04"]
["","Roczne zużycie energii","","kWh/rok","652"]