{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":52,"n_cols":7,"rows_kept":52,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXD-A"]
[]
[]
[]
[]
["","","","","","FTXD25A5V1B","FTXD35A5V1B"]
["Pobór mocy","Chłodzenie","","Nom.","kW","0.02","0.032"]
["","Grzanie","","Nom.","kW","0.023","0.032"]
["Obudowa","Kolor","","","","Biały","Biały"]
["Wymiary","Jednostka","","Wysokość","mm","286","286"]
["","","","Szerokość","mm","770","770"]
["","","","Głębokość","mm","225","225"]
["Ciężar","Jednostka","","","kg","9","9"]
["Wentylator","Przepływ powietrza","Chłodzenie","Wysoki","m³/min","9.5","11"]
["","Natężenie przepływu powietrza","Chłodzenie","Czynnik","m³/min","7.8","8.5"]
["","","","Niski","m³/min","6.3","6.8"]
["","","","Cicha praca","m³/min","4.9","5.4"]
["","","Grzanie","Wysoki","m³/min","10.5","11.5"]
["","Natężenie przepływu powietrza","Ogrzewanie","Czynnik","m³/min","8.6","9.4"]
["","","Grzanie","Niski","m³/min","7.2","7.7"]
["","","","Cicha praca","m³/min","6.1","6.3"]
["Poziom mocy akustycznej","Chłodzenie","","","dBA","57","58"]
["","Ogrzewanie","","","dBA","57","58"]
["Poziom ciśnienia akustycznego","Chłodzenie","","Wysoki","dBA","40","43"]
["","","","Czynnik","dBA","33","34"]
["","","","Niski","dBA","26","27"]
["","","","Cicha praca","dBA","19","20"]
["","Grzanie","","Wysoki","dBA","40","40"]
["","Ogrzewanie","","Czynnik","dBA","34","35"]
["","Grzanie","","Niski","dBA","28","29"]
["","","","Cicha praca","dBA","21","21"]
["Połączenia instalacji rurowej","Ciecz","","Śr. zewn.","mm","6.35","6.35"]
["","Gaz","","Śr. zewn.","mm","9.52","9.52"]
["","Spust","","","","18","18"]
["Control systems","Infrared remote control","","","","ARC480A78","ARC480A78"]
["Syst. kontroli","Pilot przewodowy","","","","BRC944B2, BRC073A1","BRC944B2, BRC073A1"]
["Standardowe akcesoria","Installation manual","","","","1","1"]
["","AAA dry-cell batteries","","","","2","2"]
["","General safety precautions","","","","1","1"]
["","Operation manual","","","","1","1"]
["","Titanium apatite deodorizing filter","","","","1","1"]
["","Silver particle filter","","","","1","1"]
["","Indoor unit fixing screws","","","","2","2"]
["","Infrared remote control","","","","1","1"]
["","Mounting plate","","","","1","1"]
["","Remote control holder","","","","1","1"]
["Zasilanie energią elektryczną","liczba faz","","","","1~","1~"]
["Zasilanie","Częstotliwość","","","Hz","50","50"]
["","Napięcie","","","V","220-240","220-240"]
["Uwagi","","","","","(1) - Chłodzenie: temp. wewn. 27°CDB, 19,0°CWB; temp. zewn. 35°CDB; długość równoważna instalacji rurowej: 5 m; różnica poziomów: 0 m","(1) - Chłodzenie: temp. wewn. 27°CDB, 19,0°CWB; temp. zewn. 35°CDB; długość równoważna instalacji rurowej: 5 m; różnica poziomów: 0 m"]
["","","","","","(2) - Grzanie: temp. wewn. 20°CDB; temp. zewnętrzna 7°CDB, 6°CWB , równoważna instalacja chłodnicza: 5 m (w poziomie)","(2) - Grzanie: temp. wewn. 20°CDB; temp. zewnętrzna 7°CDB, 6°CWB , równoważna instalacja chłodnicza: 5 m (w poziomie)"]
["","","","","","(3) - Dane elektryczne, patrz oddzielny rysunek","(3) - Dane elektryczne, patrz oddzielny rysunek"]