{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":38,"n_cols":6,"rows_kept":38,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXF-B"]
[]
[]
[]
[]
["","","","","FTXF20B5V1B","FTXF25B5V1B"]
["Poziom ciśnienia akustycznego","Grzanie","Wysoki","dBA","39","40"]
["","","Czynnik","dBA","34","34"]
["","","Cicha praca","dBA","21","21"]
["","","Niski","dBA","28","28"]
["","Chłodzenie","Czynnik","dBA","33","33"]
["","","Cicha praca","dBA","20","20"]
["","","Niski","dBA","25","26"]
["","","Wysoki","dBA","39","40"]
["Standardowe akcesoria","Instrukcja instalacji","","","1","1"]
["","Instrukcja obsługi","","","1","1"]
["","Zdalny sterownik bezprzewodowy","","","1","1"]
["","Baterie suche typu AAA","","","2","2"]
["","Uchwyt do pilota","","","1","1"]
["","Płyta montażowa","","","1","1"]
["","Śruby mocujące jednostkę wewnętrzną","","","2","2"]
["Control systems","Wired remote control","","","BRC944B2, BRC073A1","BRC944B2, BRC073A1"]
["","Infrared remote control","","","ARC470A1","ARC470A1"]
["Połączenia instalacji rurowej","Ciecz","Śr. zewn.","mm","6.35","6.35"]
["","Gaz","Śr. zewn.","mm","9.50","9.50"]
["","Spust","","","18","18"]
["Power input","Chłodzenie","Nom.","kW","0.017","0.019"]
["","Grzanie","Nom.","kW","0.020","0.020"]
["Poziom mocy akustycznej","Chłodzenie","","dBA","55","55"]
["","Ogrzewanie","","dBA","55","55"]
["Wymiary","Jednostka","Szerokość","mm","770","770"]
["","","Głębokość","mm","225","225"]
["","","Wysokość","mm","286","286"]
["Obudowa","Colour","","","Biały","Biały"]
["Ciężar","Jednostka","","kg","8.50","8.50"]
["Power supply","liczba faz","","","1~","1~"]
["","Częstotliwość","","Hz","50","50"]
["","Napięcie","","V","220-240","220-240"]