{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":27,"n_cols":6,"rows_kept":27,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXG-LW / RXLG-M"]
[]
[]
[]
[]
["","","","","FTXG25LV1BW / RXLG25M2V1B","FTXG35LV1BW / RXLG35M2V1B"]
["Wydajność chłodnicza","Min.","","kW","1.3","1.4"]
["","Maks.","","kW","4.0","4.6"]
["","Nom.","","kW","2.5 (2)","3.5 (2)"]
["Połączenia instalacji","Ciecz","Śr. zewn.","mm","6.35","6.35"]
["","Gaz","Śr. zewn.","mm","9.5","9.5"]
["","Spust","Śr. zew.","mm","18","18"]
["Efektywność nominalna","Annual energy consumption","","kWh","340","490"]
["","EER","","","3.68 (1)","3.57 (1)"]
["","COP","","","4.31 (1)","3.89 (1)"]
["","Dyrektywa na temat oznaczeń zużycia energii (klas energetycznych)","Chłodzenie","","A","A"]
["","","Ogrzewanie","","A","A"]
["Wydajność grzewcza","Nom.","","kW","4.4 (2)","5.1 (2)"]
["","Min.","","kW","1.0 (6)","1.0 (6)"]
["","Maks.","","kW","6.1, 3.6 (7)","6.7, 4.2 (7)"]
["Uwagi","","","","(1) - Wartości EER/COP według Eurovent 2012, do użytkowania tylko poza Unią Europejską","(1) - Wartości EER/COP według Eurovent 2012, do użytkowania tylko poza Unią Europejską"]
["","","","","(2) - Wydaj. znam.: (chłodzenie przy temp. 35°/27° i obciążeniu znam., grzanie przy temp. 7°/20° i obciążeniu znam.)","(2) - Wydaj. znam.: (chłodzenie przy temp. 35°/27° i obciążeniu znam., grzanie przy temp. 7°/20° i obciążeniu znam.)"]
["","","","","(3) - 220 V","(3) - 220 V"]
["","","","","(4) - 230 V","(4) - 230 V"]
["","","","","(5) - 240 V","(5) - 240 V"]
["","","","","(6) - Dla znam. minim. wydaj. grzewczej , ustawić wentylator jednostki wew. na SL","(6) - Dla znam. minim. wydaj. grzewczej , ustawić wentylator jednostki wew. na SL"]
["","","","","(7) - Maksymalna wydajność grzewcza przy temperaturze zewnętrznej -15°C","(7) - Maksymalna wydajność grzewcza przy temperaturze zewnętrznej -15°C"]