{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":35,"n_cols":8,"rows_kept":35,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXJ-AB / RXJ-M9"]
[]
[]
[]
[]
["","","","","FTXJ20A2V1BB / RXJ20M5V1B9","FTXJ25A2V1BB / RXJ25M5V1B9","FTXJ35A2V1BB  / RXJ35M5V1B9","FTXJ35A2V1BB / RXJ35M5V1B9"]
["Wydajność chłodnicza","Nom.","","kW","","","3.50"]
["Efektywność nominalna","Rocz. zużycie ener.","","kWh","","","428"]
["","EER","","","","","4.09"]
["","COP","","","","","4.04"]
["","Dyrektywa na temat oznaczeń zużycia energii (klas energetycznych)","Chłodzenie","","","","A"]
["","","Ogrzewanie","","","","A"]
["Wydajność grzewcza","Nom.","","kW","","","4.00"]
["Uwagi","","","","","","(1) - Patrz oddzielny rysunek zakresu pracy"]
["","","","","","","(2) - Dane elektryczne, patrz oddzielny rysunek"]
["","","","","","","(3) - Nominalne wydajności chłodzenia oparte są na: temperatura wewnętrzna: 27°CDB, 19°CWB, temp. zewn.: 35°CDB, równoważna dług. rur: 5 m, różnica poziomów: 0 m."]
["","","","","","","(4) - Nominalne wydajności grzewcze oparte są na: temperaturze wewnętrznej: 20°CDB; temperaturze zewnętrznej: 7°CDB, 6°CWB , równorzędnej instalacji chłodniczej: 5 m, różnicy poziomów: 0 m."]
["Jednostka zewnętrzna","","","","RXJ20M5V1B9","RXJ25M5V1B9","","RXJ35M5V1B9"]
["Wydajność chłodnicza","Nom.","","kW","2.30","2.40","","3.50"]
["Wydajność grzewcza","Nom.","","kW","2.50","3.20","","4.00"]
["Wydaj. znam.","EER","","","4.64","4.73","","4.09"]
["","COP","","","5.00","4.57","","4.04"]
["","Rocz. zużycie ener.","","kWh","248","254","","428"]
["Efektywność nominalna","Dyrektywa na temat oznaczeń zużycia energii (klas energetycznych)","Chłodzenie","","A","A","","A"]
["","","Ogrzewanie","","A","A","","A"]
["Chłodzenie pomieszczeń","Klasa efektywności energetycznej","","","A+++","A+++","","A++"]
["","Wydajność","Pdesign","kW","2.30","2.40","","3.50"]
["","SEER","","","8.73","8.64","","7.19"]
["","Roczne zużycie energii","","kWh/rok","92","97","","170"]
["Ogrzewanie pomieszczeń (przeciętny klimat)","Klasa efektywności energetycznej","","","A++","A++","","A++"]
["","Wydajność","Pdesign","kW","2.10","2.70","","3.00"]
["","SCOP/A","","","4.61","4.60","","4.60"]
["","Pdh Wydajność grzewcza w temp. -10°","","kW","1.80","2.18","","2.61"]
["","Roczne zużycie energii","","kWh/rok","638","822","","913"]
["Energy Efficiency Range","","","","A+++ ~ D","A+++ ~ D","","A+++ ~ D"]