{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":33,"n_cols":10,"rows_kept":33,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXJ-MW / 3MXM-N"]
[]
[]
[]
[]
["","","","","FTXJ20MV1BW / FTXJ20MV1BW / FTXJ20MV1BW / 3MXM40N2V1B","FTXJ20MV1BW / FTXJ20MV1BW / 3MXM40N2V1B","FTXJ20MV1BW / FTXJ20MV1BW / 3MXM52N2V1B","FTXJ20MV1BW / FTXJ20MV1BW / FTXJ20MV1BW / 3MXM52N2V1B","FTXJ20MV1BW / FTXJ20MV1BW / 3MXM68N2V1B","FTXJ20MV1BW / FTXJ20MV1BW / FTXJ20MV1BW / 3MXM68N2V1B"]
["Wydajność chłodnicza","Nom.","","kW","4.00","","4.00","5.20","4.00","6.00"]
["Efektywność nominalna","Annual energy consumption","","kWh","467","","471","593","457","787"]
["","EER","","","4.28","","4.25","4.38","4.38","3.81"]
["","COP","","","4.32","","4.05","4.42","4.04","3.88"]
["","Dyrektywa na temat oznaczeń zużycia energii (klas energetycznych)","Chłodzenie","","A","","A","A","A","A"]
["","","Ogrzewanie","","A","","A","A","A","A"]
["Wydajność grzewcza","Nom.","","kW","4.60","","6.80","6.80","6.50","7.80"]
["Wydajność chłodnicza","Nom.","","kW","","4.00"]
["Wydajność grzewcza","Nom.","","kW","","4.60"]
["Wydaj. znam.","EER","","","","4.15"]
["","COP","","","","3.95"]
["","Rocz. zużycie ener.","","kWh","","482"]
["Efektywność nominalna","Dyrektywa na temat oznaczeń zużycia energii (klas energetycznych)","Chłodzenie","","","A"]
["","","Ogrzewanie","","","A"]
["Chłodzenie pomieszczeń","Klasa efektywności energetycznej","","","","A++"]
["","Wydajność","Pdesign","kW","","4.00"]
["","SEER","","","","7.62"]
["","Roczne zużycie energii","","kWh/rok","","164"]
["Ogrzewanie pomieszczeń (przeciętny klimat)","Klasa efektywności energetycznej","","","","A+"]
["","Wydajność","Pdesign","kW","","4.80"]
["","SCOP/A","","","","4.11"]
["","Pdh Wydajność grzewcza w temp. -10°","","kW","","3.58"]
["","Roczne zużycie energii","","kWh/rok","","1632"]
["Uwagi","","","","","(1) - Nominalne wydajności chłodzenia oparte są na: temp. wewnętrzna: 27°CDB, 19°CWB, temp. zewn.: 35°CDB, równoważna dług. rur: 5 m, różnica poziomów: 0 m."]
["","","","","","(2) - Nominalne wydajności grzewcze oparte są na: temperaturze wewnętrznej: 20°CDB; temperaturze zewnętrznej: 7°CDB, 6°CWB , równorzędnej instalacji chłodniczej: 5 m, różnicy poziomów: 0 m."]
["","","","","","(3) - Patrz oddzielny rysunek zakresu pracy"]
["","","","","","(4) - Dane elektryczne, patrz oddzielny rysunek"]