{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":37,"n_cols":9,"rows_kept":37,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXK-AS"]
[]
[]
[]
[]
["","","","","","FTXK25AV1BS","FTXK35AV1BS","FTXK50AV1BS","FTXK60AV1BS"]
["Wentylator","Przepływ powietrza","Chłodzenie","Nom.","m³/min","7.68","7.98","13.32","16.56"]
["Poziom ciśnienia akustycznego","Chłodzenie","","Nom.","dBA","34","34","38","41"]
["Wentylator","Przepływ powietrza","Grzanie","Nom.","m³/min","7.68","7.98","13.32","16.56"]
["Poziom ciśnienia akustycznego","Grzanie","","Nom.","dBA","34","34","38","41"]
["Obudowa","Kolor","","","","Srebrny","Srebrny","Srebrny","Srebrny"]
["Wymiary","Jednostka","","Wysokość","mm","297","297","320","320"]
["","","","Szerokość","mm","890","890","1172","1172"]
["","","","Głębokość","mm","210","210","242","242"]
["Ciężar","Jednostka","","","kg","9.0","9.0","14.0","14.0"]
["Wentylator","Przepływ powietrza","Chłodzenie","Wysoki","m³/min","9.78","10.14","15.00","18.54"]
["","","","Niski","m³/min","6.06","6.54","11.82","14.34"]
["","","","Cicha praca","m³/min","4.68","4.68","10.62","12.36"]
["","","Grzanie","Wysoki","m³/min","9.78","10.14","15.00","18.54"]
["","","","Niski","m³/min","6.06","6.54","11.82","14.34"]
["","","","Cicha praca","m³/min","4.68","4.68","10.62","12.36"]
["Poziom mocy akustycznej","Chłodzenie","","","dBA","53","54","55","61"]
["","Ogrzewanie","","","dBA","53","54","55","61"]
["Poziom ciśnienia akustycznego","Chłodzenie","","Bardzo wysoki","dBA","41","42","44","46"]
["","","","Wysoki","dBA","40","41","40","43"]
["","","","Niski","dBA","29","30","35","37"]
["","","","Cicha praca","dBA","21","22","32","33"]
["","Grzanie","","Wysoki","dBA","40","41","40","43"]
["","","","Niski","dBA","29","30","35","37"]
["","","","Cicha praca","dBA","21","22","32","33"]
["Czynnik chłodniczy","GWP","","","","2087.5","2087.5","2087.5","2087.5"]
["Połączenia instalacji rurowej","Ciecz","","Śr. zewn.","mm","6.35","6.35","6.35","6.35"]
["","Gaz","","Śr. zewn.","mm","9.52","9.52","12.70","15.90"]
["Zasilanie energią elektryczną","Nazwa","","","","V1","V1","V1","V1"]
["","liczba faz","","","","1~","1~","1~","1~"]
["Zasilanie","Częstotliwość","","","Hz","50","50","50","50"]
["","Napięcie","","","V","220-240","220-240","220-240","220-240"]