{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":43,"n_cols":6,"rows_kept":43,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXLS-K3"]
[]
[]
[]
[]
["","","","","FTXLS25K3V1B","FTXLS35K3V1B"]
["Poziom ciśnienia akustycznego","Grzanie","Wysoki","dBA","47","47"]
["","","Cicha praca","dBA","19","19"]
["","","Niski","dBA","23","23"]
["","Chłodzenie","Cicha praca","dBA","21","21"]
["","","Niski","dBA","33","33"]
["","","Wysoki","dBA","45","45"]
["","","Nom.","dBA","37","36"]
["","Chłodzenie","Nom.","dBA","39","39"]
["Standardowe akcesoria","Instrukcja instalacji","","","1","1"]
["","Instrukcja obsługi","","","1","1"]
["","Zdalny sterownik bezprzewodowy","","","1","1"]
["","Baterie","","","2","2"]
["","Uchwyt do pilota","","","1","1"]
["","Płyta montażowa","","","1","1"]
["","Tytanowo-apatytowy fotokatalityczny filtr oczyszczający powietrze","","","2","2"]
["","Śruby mocujące jednostkę wewnętrzną","","","2","2"]
["Systemy sterujące","Infrared remote control","","","ARC466A9","ARC466A9"]
["Połączenia instalacji rurowej","Ciecz","Śr. zewn.","mm","6.35","6.35"]
["","Gaz","Śr. zewn.","mm","9.5","9.5"]
["","Spust","","","18","18"]
["Power input","Chłodzenie","Nom.","kW","0.024 (2), 0.024 (3), 0.024 (4)","0.024 (2), 0.024 (3), 0.024 (4)"]
["","Grzanie","Nom.","kW","0.030 (2), 0.030 (3), 0.030 (4)","0.030 (2), 0.030 (3), 0.030 (4)"]
["Sound power level","Chłodzenie","","dBA","59","59"]
["","Ogrzewanie","","dBA","62","62"]
["Wymiary","Jednostka","Szerokość","mm","900","900"]
["","","Głębokość","mm","215","215"]
["","","Wysokość","mm","298","298"]
["Casing","Colour","","","Biały","Biały"]
["Ciężar","Jednostka","","kg__","12","12"]
["Power supply","Phase","","","1~","1~"]
["","Częstotliwość","","Hz","50","50"]
["","Nazwa","","","V1","V1"]
["","Napięcie","","V","220-240","220-240"]
["Uwagi","","","","(1) - Po podłączeniu do jednostki zewnętrznej w systemie multi, patrz specyfikacje podłączanej jednostki zewnętrznej multi.","(1) - Po podłączeniu do jednostki zewnętrznej w systemie multi, patrz specyfikacje podłączanej jednostki zewnętrznej multi."]
["","","","","(2) - 220 V","(2) - 220 V"]
["","","","","(3) - 230 V","(3) - 230 V"]
["","","","","(4) - 240 V","(4) - 240 V"]