{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":41,"n_cols":9,"rows_kept":41,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXM-K"]
[]
[]
[]
[]
["","","","","FTXM20K3V1B (Archived)","FTXM25K3V1B (Archived)","FTXM35K3V1B (Archived)","FTXM42K3V1B (Archived)","FTXM50K3V1B (Archived)"]
["Poziom ciśnienia akustycznego","Grzanie","Wysoki","dBA","40","41","45","45","47"]
["","","Cicha praca","dBA","19","19","19","22","24"]
["","","Niski","dBA","27","27","29","33","34"]
["","Chłodzenie","Cicha praca","dBA","19","19","19","21","23"]
["","","Niski","dBA","24","25","29","33","34"]
["","","Wysoki","dBA","40","41","45","45","46"]
["","","Nom.","dBA","34","34","39","39","40"]
["","Chłodzenie","Nom.","dBA","32","33","37","39","40"]
["Standardowe akcesoria","Instrukcja obsługi","","","1","1","1","1","1"]
["","Instrukcja instalacji","","","1","1","1","1","1"]
["","Zdalny sterownik bezprzewodowy","","","1","1","1","1","1"]
["","Baterie","","","2","2","2","2","2"]
["","Płyta montażowa","","","1","1","1","1","1"]
["","Śruby mocujące jednostkę wewnętrzną","","","2","2","2","2","2"]
["","Tytanowo-apatytowy fotokatalityczny filtr oczyszczający powietrze","","","2","2","2","2","2"]
["","Uchwyt do pilota","","","1","1","1","1","1"]
["Control systems","Infrared remote control","","","ARC466A6","ARC466A6","ARC466A9","ARC466A9","ARC466A9"]
["Połączenia instalacji","Ciecz","Śr. zewn.","mm","6.35","6.35","6.35","6.35","6.35"]
["","Gaz","Śr. zewn.","mm","9.5","9.5","9.5","12.7","12.7"]
["","Spust","","","18","18","18","18","18"]
["Sound power level","Chłodzenie","","dBA","56","57","59","59","60"]
["","Ogrzewanie","","dBA","56","57","59","59","60"]
["Wymiary","Jednostka","Szerokość","mm","780","780","900","900","900"]
["","","Głębokość","mm","215","215","215","215","215"]
["","","Wysokość","mm","289","289","298","298","298"]
["Obudowa","Kolor","","","Biały","Biały","Biały","Biały","Biały"]
["Ciężar","Jednostka","","kg","8","8","11","11","11"]
["Power supply","liczba faz","","","1~","1~","1~","1~","1~"]
["","Częstotliwość","","Hz","50","50","50","50","50"]
["","Nazwa","","","V1","V1","V1","V1","V1"]
["","Napięcie","","V","220-240","220-240","220-240","220-240","220-240"]
["Uwagi","","","","(1) - SL: poziom cichego wentylatora ustawienia szybkości przepływu powietrza","(1) - SL: poziom cichego wentylatora ustawienia szybkości przepływu powietrza","(1) - SL: poziom cichego wentylatora ustawienia szybkości przepływu powietrza","(1) - SL: poziom cichego wentylatora ustawienia szybkości przepływu powietrza","(1) - SL: poziom cichego wentylatora ustawienia szybkości przepływu powietrza"]
["","","","","(2) - 220 V","(2) - 220 V","(2) - 220 V","(2) - 220 V","(2) - 220 V"]
["","","","","(3) - 230 V","(3) - 230 V","(3) - 230 V","(3) - 230 V","(3) - 230 V"]
["","","","","(4) - 240 V","(4) - 240 V","(4) - 240 V","(4) - 240 V","(4) - 240 V"]