{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":25,"n_cols":8,"rows_kept":25,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXM-R / 3MXM-N8"]
[]
[]
[]
[]
["","","","","FTXM20R5V1B / FTXM20R5V1B / 3MXM40N2V1B8","FTXM20R2V1B / FTXM20R2V1B / 3MXM40N2V1B8","FTXM25R2V1B / FTXM25R2V1B / 3MXM52N2V1B8","FTXM25R5V1B / FTXM25R5V1B / 3MXM52N2V1B8"]
["Wydajność chłodnicza","Nom.","","kW","4.00","4.00","5.0","5.0"]
["Efektywność nominalna","Rocz. zużycie ener.","","kWh","420","420","515","515"]
["","EER","","","4.76","4.76","4.85","4.85"]
["","COP","","","4.73","4.73","4.45","4.45"]
["","Dyrektywa na temat oznaczeń zużycia energii (klas energetycznych)","Chłodzenie","","A","A","A","A"]
["","","Ogrzewanie","","A","A","A","A"]
["Chłodzenie pomieszczeń","Roczne zużycie energii","","kWh/rok","","","204","204"]
["","Wydajność","Pdesign","kW","","","5.00","5.00"]
["Ogrzewanie pomieszczeń (przeciętny klimat)","Wydajność","Pdesign","kW","","","4.80","4.80"]
["","Roczne zużycie energii","","kWh/rok","","","1,533","1,533"]
["Wydajność grzewcza","Nom.","","kW","4.60","4.60","6.80","6.80"]
["Uwagi","","","","(1) - Nominalne wydajności chłodzenia oparte są na: temp. wewnętrzna: 27°CDB, 19°CWB, temp. zewn.: 35°CDB, równoważna dług. rur: 5 m, różnica poziomów: 0 m.","(1) - Nominalne wydajności chłodzenia oparte są na: temp. wewnętrzna: 27°CDB, 19°CWB, temp. zewn.: 35°CDB, równoważna dług. rur: 5 m, różnica poziomów: 0 m.","(1) - Nominalne wydajności chłodzenia oparte są na: temp. wewnętrzna: 27°CDB, 19°CWB, temp. zewn.: 35°CDB, równoważna dług. rur: 5 m, różnica poziomów: 0 m.","(1) - Nominalne wydajności chłodzenia oparte są na: temp. wewnętrzna: 27°CDB, 19°CWB, temp. zewn.: 35°CDB, równoważna dług. rur: 5 m, różnica poziomów: 0 m."]
["","","","","(2) - Nominalne wydajności grzewcze oparte są na: temperaturze wewnętrznej: 20°CDB; temperaturze zewnętrznej: 7°CDB, 6°CWB , równorzędnej instalacji chłodniczej: 5 m, różnicy poziomów: 0 m.","(2) - Nominalne wydajności grzewcze oparte są na: temperaturze wewnętrznej: 20°CDB; temperaturze zewnętrznej: 7°CDB, 6°CWB , równorzędnej instalacji chłodniczej: 5 m, różnicy poziomów: 0 m.","(2) - Nominalne wydajności grzewcze oparte są na: temperaturze wewnętrznej: 20°CDB; temperaturze zewnętrznej: 7°CDB, 6°CWB , równorzędnej instalacji chłodniczej: 5 m, różnicy poziomów: 0 m.","(2) - Nominalne wydajności grzewcze oparte są na: temperaturze wewnętrznej: 20°CDB; temperaturze zewnętrznej: 7°CDB, 6°CWB , równorzędnej instalacji chłodniczej: 5 m, różnicy poziomów: 0 m."]
["","","","","(3) - Patrz oddzielny rysunek zakresu pracy","(3) - Patrz oddzielny rysunek zakresu pracy","(3) - Patrz oddzielny rysunek zakresu pracy","(3) - Patrz oddzielny rysunek zakresu pracy"]
["","","","","(4) - Dane elektryczne, patrz oddzielny rysunek","(4) - Dane elektryczne, patrz oddzielny rysunek","(4) - Dane elektryczne, patrz oddzielny rysunek","(4) - Dane elektryczne, patrz oddzielny rysunek"]
["Chłodzenie pomieszczeń","SEER","","","","","8.59","8.59"]
["","Klasa efektywności energetycznej","","","","","A+++","A+++"]
["Ogrzewanie pomieszczeń (przeciętny klimat)","SCOP/A","","","","","4.38","4.38"]
["","Klasa efektywności energetycznej","","","","","A+","A+"]