{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":25,"n_cols":5,"rows_kept":25,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXS-G / RXS-F8"]
[]
[]
[]
[]
["","","","","FTXS71GV1B / RXS71FAV1B8"]
["Wydajność chłodnicza","Min.","","kW","2.3"]
["","Maks.","","kW","8.5"]
["","Nom.","","kW","7.10"]
["Połączenia instalacji rurowej","Ciecz","Śr. zewn.","mm","6.35"]
["","Gaz","Śr. zewn.","mm","15.9"]
["","Spust","Śr. zew.","mm","18"]
["Efektywność nominalna","Annual energy consumption","","kWh","1,175"]
["","EER","","","3.02"]
["","COP","","","3.22"]
["","Dyrektywa na temat oznaczeń zużycia energii (klas energetycznych)","Chłodzenie","","B"]
["","","Ogrzewanie","","C"]
["Wydajność grzewcza","Nom.","","kW","8.20"]
["","Min.","","kW","2.3"]
["","Maks.","","kW","10.2"]
["Uwagi","","","","(1) - Wartości EER/COP według Eurovent 2012, do użytkowania tylko poza Unią Europejską"]
["","","","","(2) - 220 V"]
["","","","","(3) - 230 V"]
["","","","","(4) - 240 V"]
["","","","","(5) - Wydaj. znam.: (chłodzenie przy temp. 35°/27° i obciążeniu znam., grzanie przy temp. 7°/20° i obciążeniu znam.)"]