{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":85,"n_cols":12,"rows_kept":85,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXS-G"]
[]
[]
[]
[]
["","","","","","FTXS20G2V1B","FTXS25G2V1B","FTXS35G2V1B","FTXS42G2V1B","FTXS50G2V1B","FTXS60GV1B","FTXS71GV1B"]
["Poziom ciśnienia akustycznego","Grzanie","","Wysoki","dBA","38","39","42","42","44","","46"]
["","","","Cicha praca","dBA","25","25","26","30","31","","34"]
["","","","Niski","dBA","28","28","29","33","34","","37"]
["","Chłodzenie","","Cicha praca","dBA","22","22","23","30","31","","34"]
["","","","Niski","dBA","25","25","26","33","34","","37"]
["","","","Wysoki","dBA","38","38","42","42","43","","46"]
["","","","Nom.","dBA","33","34","36","38","39","","42"]
["","Chłodzenie","","Nom.","dBA","32","32","34","38","39","","42"]
["Standardowe akcesoria","Tytanowo-apatytowy fotokatalityczny filtr oczyszczający powietrze","","","","2","2","2","2","2"]
["","Instrukcja obsługi","","","","1","1","1","1","1","","1"]
["","Instrukcja instalacji","","","","1","1","1","1","1","","1"]
["","Pilot bezprzewodowy","","","","1","1","1","1","1","","1"]
["","Baterie","","","","2","2","2","2","2","","2"]
["","Uchwyt do pilota","","","","1","1","1","1","1","","1"]
["","Śruby mocujące jednostkę wewnętrzną","","","","2","2","2","2","2","","2"]
["","Płyta montażowa","","","","1","1","1","1","1","","1"]
["Syst. kontroli","Infrared remote control","","","","","","","","","","ARC452A3"]
["Połączenia instalacji","Ciecz","","Śr. zewn.","mm","6.35","6.35","6.35","6.35","6.35","","6.35"]
["","Gaz","","Śr. zewn.","mm","9.52","9.52","9.52","9.52","12.70","","15.9"]
["","Spust","","","","18","18","18","18","18","","18"]
["Power input","Chłodzenie","","Nom.","kW","","","","","","","0.045 (2), 0.045 (3), 0.045 (4)"]
["","Grzanie","","Nom.","kW","","","","","","","0.060 (2), 0.060 (3), 0.060 (4)"]
["Sound power level","Chłodzenie","","","dBA","54","54","58","58","59","","63"]
["","Ogrzewanie","","","dBA","54","55","58","58","60","","62"]
["Wymiary","Jednostka","","Szerokość","mm","800","800","800","800","800","","1,050"]
["","","","Głębokość","mm","215","215","215","215","215","","250"]
["","","","Wysokość","mm","295","295","295","295","295","","290"]
["Obudowa","Kolor","","","","Biały","Biały","Biały","Biały","Biały","","Biały"]
["Ciężar","Jednostka","","","kg","9","9","10","10","10","","12"]
["Power supply","liczba faz","","","","1~","1~","1~","1~","1~","","1~"]
["","Częstotliwość","","","Hz","50","50","50","50","50","","50"]
["","Nazwa","","","","V1","V1","V1","V1","V1","","V1"]
["","Napięcie","","","V","220-240","220-240","220-240","220-240","220-240","","220-240"]
["Uwagi","","","","","(1) - 220 V","(1) - 220 V","(1) - 220 V","(1) - 220 V","(1) - 220 V","(1) - 220 V","(1) - SL: poziom cichego wentylatora ustawienia szybkości przepływu powietrza"]
["","","","","","(2) - 230 V","(2) - 230 V","(2) - 230 V","(2) - 230 V","(2) - 230 V","(2) - 230 V","(2) - 220 V"]
["","","","","","(3) - 240 V","(3) - 240 V","(3) - 240 V","(3) - 240 V","(3) - 240 V","(3) - 240 V","(3) - 230 V"]
["Wentylator","Przepływ powietrza","Chłodzenie","Nom.","m³/min","","","","","","16.0"]
["Poziom ciśnienia akustycznego","Chłodzenie","","Nom.","dBA","","","","","","41"]
["Wentylator","Przepływ powietrza","Grzanie","Nom.","m³/min","","","","","","14.9"]
["Poziom ciśnienia akustycznego","Grzanie","","Nom.","dBA","","","","","","40"]
["Pobór mocy","Chłodzenie","","Nom.","kW","","","","","","0.040 (4) (2) (3), 0.040 (4) (2) (3), 0.040 (4) (2) (3)"]
["","Grzanie","","Nom.","kW","","","","","","0.045 (4) (2) (3), 0.045 (4) (2) (3), 0.045 (4) (2) (3)"]
["Obudowa","Kolor","","","","","","","","","Biały"]
["Wymiary","Jednostka","","Wysokość","mm","","","","","","290"]
["","","","Szerokość","mm","","","","","","1050"]
["","","","Głębokość","mm","","","","","","250"]
["Ciężar","Jednostka","","","kg","","","","","","12"]
["Wentylator","Przepływ powietrza","Chłodzenie","Wysoki","m³/min","","","","","","16.0"]
["","","","Niski","m³/min","","","","","","11.3"]
["","","","Cicha praca","m³/min","","","","","","10.1"]
["","","Grzanie","Wysoki","m³/min","","","","","","17.2"]
["","","","Niski","m³/min","","","","","","12.6"]
["","","","Cicha praca","m³/min","","","","","","11.3"]
["Poziom mocy akustycznej","Chłodzenie","","","dBA","","","","","","60"]
["","Ogrzewanie","","","dBA","","","","","","59"]
["Poziom ciśnienia akustycznego","Chłodzenie","","Wysoki","dBA","","","","","","45"]
["","","","Niski","dBA","","","","","","36"]
["","","","Cicha praca","dBA","","","","","","33"]
["","Grzanie","","Wysoki","dBA","","","","","","44"]
["","","","Niski","dBA","","","","","","35"]
["","","","Cicha praca","dBA","","","","","","32"]
["Połączenia instalacji rurowej","Ciecz","","Śr. zewn.","mm","","","","","","6.35"]
["","Gaz","","Śr. zewn.","mm","","","","","","12.7"]
["","Spust","","","","","","","","","18"]
["Syst. kontroli","Pilot na podczerwień","","","","","","","","","ARC452A3"]
["Standardowe akcesoria","Installation manual","","","","","","","","","1"]
["","Wireless remote control","","","","","","","","","1"]
["","Operation manual","","","","","","","","","1"]
["","Batteries","","","","","","","","","2"]
["","Indoor unit fixing screws","","","","","","","","","2"]
["","Mounting plate","","","","","","","","","1"]
["","Remote control holder","","","","","","","","","1"]
["","Titanium apatite photocatalytic air purification filter","","","","","","","","","2"]
["Zasilanie energią elektryczną","Nazwa","","","","","","","","","V1"]
["","liczba faz","","","","","","","","","1~"]
["Zasilanie","Częstotliwość","","","Hz","","","","","","50"]
["","Napięcie","","","V","","","","","","220-240"]
["Standardowe akcesoria","Tytanowo-apatytowy fotokatalityczny filtr oczyszczający powietrze bez ramy","","","","","","","","","","2"]
["Uwagi","","","","","","","","","","","(4) - 240 V"]