{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":91,"n_cols":15,"rows_kept":91,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXS-K"]
[]
[]
[]
[]
["","","","","","FTXS20K2V1B","FTXS20K3V1B","FTXS25K2V1B","FTXS25K3V1B","FTXS35K2V1B","FTXS35K3V1B","FTXS42K2V1B","FTXS42K3V1B","FTXS50K2V1B","FTXS50K3V1B"]
["Poziom ciś. akust.","Grzanie","","Wysoki","dBA","40","","","","","","45"]
["","","","Cicha praca","dBA","19","","","","","","22"]
["","","","Niski","dBA","27","","","","","","33"]
["","Chłodzenie","","Cicha praca","dBA","19","","","","","","21"]
["","","","Niski","dBA","24","","","","","","33"]
["","","","Wysoki","dBA","40","","","","","","45"]
["","","","Nom.","dBA","34","","","","","","39"]
["","Chłodzenie","","Nom.","dBA","32","","","","","","39"]
["Standardowe akcesoria","Instrukcja instalacji","","","","1","","","","","","1"]
["","Instrukcja obsługi","","","","1","","","","","","1"]
["","Pilot bezprzewodowy","","","","1","","","","","","1"]
["","Baterie","","","","2","","","","","","2"]
["","Uchwyt do pilota","","","","1","","","","","","1"]
["","Płyta montażowa","","","","1","","","","","","1"]
["","Śruby mocujące jednostkę wewnętrzną","","","","2","","","","","","2"]
["","Tytanowo-apatytowy fotokatalityczny filtr oczyszczający powietrze","","","","2","","","","","","2"]
["Syst. kontroli","Infrared remote control","","","","ARC466A6","","","","","","ARC466A6"]
["Połączenia instalacji","Ciecz","","Śr. zewn.","mm","6.35","","","","","","6.35"]
["","Gaz","","Śr. zewn.","mm","9.5","","","","","","9.5"]
["","Spust","","","","18","","","","","","18"]
["Power input","Chłodzenie","","Nom.","kW","0.04","","","","","","0.024 (2), 0.024 (3), 0.024 (4)"]
["","Grzanie","","Nom.","kW","0.04","","","","","","0.030 (2), 0.030 (3), 0.030 (4)"]
["Poziom mocy akustycznej","Chłodzenie","","","dBA","58","","","","","","59"]
["","Ogrzewanie","","","dBA","58","","","","","","59"]
["Wymiary","Jednostka","","Szerokość","mm","780","","","","","","900"]
["","","","Głębokość","mm","215","","","","","","215"]
["","","","Wysokość","mm","289","","","","","","298"]
["Obudowa","Colour","","","","Biały","","","","","","Biały"]
["Ciężar","Jednostka","","","kg","8","","","","","","11"]
["Power supply","Phase","","","","1~","","","","","","1~"]
["","Częstotliwość","","","Hz","50","","","","","","50"]
["","Nazwa","","","","V1","","","","","","V1"]
["","Napięcie","","","V","220-240","","","","","","220-240"]
["Uwagi","","","","","(1) - 220 V","(1) - 220 V","(1) - 220 V","(1) - 220 V","(1) - 220 V","(1) - 220 V","(1) - Po podłączeniu do jednostki zewnętrznej w systemie multi, patrz specyfikacje podłączanej jednostki zewnętrznej multi.","(1) - 220 V","(1) - 220 V","(1) - 220 V"]
["","","","","","(2) - 230 V","(2) - 230 V","(2) - 230 V","(2) - 230 V","(2) - 230 V","(2) - 230 V","(2) - 220 V","(2) - 230 V","(2) - 230 V","(2) - 230 V"]
["","","","","","(3) - 240 V","(3) - 240 V","(3) - 240 V","(3) - 240 V","(3) - 240 V","(3) - 240 V","(3) - 230 V","(3) - 240 V","(3) - 240 V","(3) - 240 V"]
["Pobór mocy","Chłodzenie","","Nom.","kW","","0.040, 0.040, 0.040","0.04","0.040 (3) (1) (2), 0.040 (3) (1) (2), 0.040 (3) (1) (2)","0.026 (3) (4) (2), 0.026 (3) (4) (2), 0.026 (3) (4) (2)","0.026 (1) (3) (2), 0.026 (1) (3) (2), 0.026 (1) (3) (2)","","0.024, 0.024, 0.024","0.026 (4) (2) (3), 0.026 (4) (2) (3), 0.026 (4) (2) (3)","0.026 (1) (2) (3), 0.026 (1) (2) (3), 0.026 (1) (2) (3)"]
["","Grzanie","","Nom.","kW","","0.040, 0.040, 0.040","0.04","0.040 (2) (3) (1), 0.040 (2) (3) (1), 0.040 (2) (3) (1)","0.028 (2) (4) (3), 0.028 (2) (4) (3), 0.028 (2) (4) (3)","0.028 (1) (3) (2), 0.028 (1) (3) (2), 0.028 (1) (3) (2)","","0.030, 0.030, 0.030","0.032 (2) (4) (3), 0.032 (2) (4) (3), 0.032 (2) (4) (3)","0.032 (2) (1) (3), 0.032 (2) (1) (3), 0.032 (2) (1) (3)"]
["Obudowa","Kolor","","","","","Biały","Biały","Biały","Biały","Biały","","Biały","Biały","Biały"]
["Wymiary","Jednostka","","Wysokość","mm","","215","289","215","298","215","","215","298","215"]
["","","","Szerokość","mm","","780","780","780","900","900","","900","900","900"]
["","","","Głębokość","mm","","289","215","289","215","298","","298","215","298"]
["Ciężar","Jednostka","","","kg","","8.00","8","8.00","11","11.0","","11.0","11","11.0"]
["Wentylator","Przepływ powietrza","Chłodzenie","Wysoki","m³/min","","8.8","9.1","9.1","11.2","11.2","","11.2","11.9","11.9"]
["","Natężenie przepływu powietrza","Chłodzenie","Czynnik","m³/min","","6.7","7.0","7.0","","8.5","","9.1","","9.6"]
["","","","Niski","m³/min","","4.7","5.0","5.0","5.8","5.8","","7.0","7.4","7.4"]
["","","","Cicha praca","m³/min","","3.9","3.9","3.9","4.1","4.1","","4.1","4.5","4.5"]
["","","Grzanie","Wysoki","m³/min","","9.5","10.0","10.0","12.1","12.1","","12.4","13.3","13.3"]
["","Natężenie przepływu powietrza","Ogrzewanie","Czynnik","m³/min","","7.8","8.0","8.0","","9.3","","10.0","","10.8"]
["","","Grzanie","Niski","m³/min","","6.0","6.0","6.0","6.5","6.5","","7.8","8.4","8.4"]
["","","","Cicha praca","m³/min","","4.3","4.3","4.3","4.2","4.2","","5.2","5.5","5.5"]
["Poziom mocy akustycznej","Chłodzenie","","","dBA","","58","58","58","59","59","","59","60","60"]
["","Ogrzewanie","","","dBA","","58","58","58","59","59","","59","60","60"]
["Poziom ciśnienia akustycznego","Chłodzenie","","Wysoki","dBA","","40","41","41","45","45","","45","46","46"]
["","","","Czynnik","dBA","","32","33","33","","37","","39","","40"]
["","","","Niski","dBA","","24","25","25","29","29","","33","34","34"]
["","","","Cicha praca","dBA","","19","19","19","19","19","","21","23","23"]
["","Grzanie","","Wysoki","dBA","","40","41","41","45","45","","45","47","47"]
["","Ogrzewanie","","Czynnik","dBA","","34","34","34","","39","","39","","40"]
["","Grzanie","","Niski","dBA","","27","27","27","29","29","","33","34","34"]
["","","","Cicha praca","dBA","","19","19","19","19","19","","22","24","24"]
["Połączenia instalacji rurowej","Ciecz","","Śr. zewn.","mm","","6.35","6.35","6.35","6.35","6.35","","6.35","6.35","6.35"]
["","Gaz","","Śr. zewn.","mm","","9.50","9.5","9.50","9.5","9.50","","9.50","12.7","12.7"]
["","Spust","","","","","18","18","18","18","18","","18","18","18"]
["Syst. kontroli","Infrared remote control","","","","","ARC466A6","","","","","","ARC466A9"]
["Standardowe akcesoria","Installation manual","","","","","1","1","1","1","1","","1","1","1"]
["","Wireless remote control","","","","","1","1","1","1","1","","1","1","1"]
["","AAA dry-cell batteries","","","","","2","","2","","2","","2","","2"]
["","Operation manual","","","","","1","1","1","1","1","","1","1","1"]
["","Titanium apatite deodorizing filter","","","","","2","","2","","2","","2","","2"]
["","Indoor unit fixing screws","","","","","2","2","2","2","2","","2","2","2"]
["","Mounting plate","","","","","1","1","1","1","1","","1","1","1"]
["","Remote control holder","","","","","1","1","1","1","1","","1","1","1"]
["Zasilanie energią elektryczną","Nazwa","","","","","V1","V1","V1","V1","V1","","V1","V1","V1"]
["","liczba faz","","","","","1~","1~","1~","1~","1~","","1~","1~","1~"]
["Zasilanie","Częstotliwość","","","Hz","","50","50","50","50","50","","50","50","50"]
["","Napięcie","","","V","","220-240","220-240","220-240","220-240","220-240","","220-240","220-240","220-240"]
["Wentylator","Przepływ powietrza","Chłodzenie","Nom.","m³/min","","","9.1","","11.2","","","","11.9"]
["Poziom ciśnienia akustycznego","Chłodzenie","","Nom.","dBA","","","33","","37","","","","40"]
["Wentylator","Przepływ powietrza","Grzanie","Nom.","m³/min","","","8.0","","9.3","","","","10.8"]
["Poziom ciśnienia akustycznego","Grzanie","","Nom.","dBA","","","34","","39","","","","40"]
["Syst. kontroli","Pilot na podczerwień","","","","","","ARC466A6","ARC466A6","ARC466A6","ARC466A9","","","ARC466A6","ARC466A9"]
["Standardowe akcesoria","Batteries","","","","","","2","","2","","","","2"]
["","Titanium apatite photocatalytic air purification filter","","","","","","2","","2","","","","2"]
["Uwagi","","","","","","","","","","","(4) - 240 V"]