{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":50,"n_cols":6,"rows_kept":50,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXTA-CW"]
[]
[]
[]
[]
["","","","","","FTXTA30C2V1BW"]
["Pobór mocy","Chłodzenie","","Nom.","kW","0.023"]
["","Grzanie","","Nom.","kW","0.022"]
["Obudowa","Kolor","","","","Biały"]
["Wymiary","Jednostka","","Wysokość","mm","295"]
["","","","Szerokość","mm","798"]
["","","","Głębokość","mm","189"]
["Ciężar","Jednostka","","","kg","12"]
["Wentylator","Przepływ powietrza","Chłodzenie","Wysoki","m³/min","13.1"]
["","Natężenie przepływu powietrza","Chłodzenie","Czynnik","m³/min","9"]
["","","","Niski","m³/min","6"]
["","","","Cicha praca","m³/min","4.9"]
["","","Grzanie","Wysoki","m³/min","12.3"]
["","Natężenie przepływu powietrza","Ogrzewanie","Czynnik","m³/min","8.2"]
["","","Grzanie","Niski","m³/min","5.8"]
["","","","Cicha praca","m³/min","5"]
["Poziom mocy akustycznej","Chłodzenie","","","dBA","60"]
["","Ogrzewanie","","","dBA","60"]
["Poziom ciśnienia akustycznego","Chłodzenie","","Wysoki","dBA","43"]
["","","","Czynnik","dBA","32"]
["","","","Niski","dBA","25"]
["","","","Cicha praca","dBA","20"]
["","Grzanie","","Wysoki","dBA","41"]
["","Ogrzewanie","","Czynnik","dBA","31"]
["","Grzanie","","Niski","dBA","24"]
["","","","Cicha praca","dBA","19"]
["Czynnik chłodniczy","GWP","","","","675"]
["Połączenia instalacji rurowej","Ciecz","","Śr. zewn.","mm","6.35"]
["","Gaz","","Śr. zewn.","mm","9.5"]
["","Spust","","","","18"]
["Syst. kontroli","Infrared remote control","","","","ARC466A84"]
["Syst. kontroli","Pilot przewodowy","","","","BRC073A4"]
["Standardowe akcesoria","Installation manual","","","","1"]
["","Wireless remote control","","","","1"]
["","Screw cover","","","","2"]
["","AAA dry-cell batteries","","","","2"]
["","General safety precautions","","","","1"]
["","Operation manual","","","","1"]
["","Titanium apatite deodorizing filter","","","","1"]
["","Silver particle filter","","","","1"]
["","Remote control holder","","","","1"]
["","Screw bag","","","","1"]
["Zasilanie energią elektryczną","liczba faz","","","","1~"]
["Zasilanie","Częstotliwość","","","Hz","50"]
["","Napięcie","","","V","220-240"]