{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":55,"n_cols":7,"rows_kept":55,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXTM-A"]
[]
[]
[]
[]
["","","","","","FTXTM30A2V1B","FTXTM40A2V1B"]
["Pobór mocy","Chłodzenie","","Nom.","kW","0.029","0.053"]
["","Grzanie","","Nom.","kW","0.024","0.06"]
["Obudowa","Kolor","","","","Biały","Biały"]
["Wymiary","Jednostka","","Wysokość","mm","298","298"]
["","","","Szerokość","mm","804","997"]
["","","","Głębokość","mm","252","292"]
["Ciężar","Jednostka","","","kg","12","15"]
["Wentylator","Przepływ powietrza","Chłodzenie","Wysoki","m³/min","13.2","15.1"]
["","Natężenie przepływu powietrza","Chłodzenie","Czynnik","m³/min","8.1","9.2"]
["","","","Niski","m³/min","5.6","5.6"]
["","","","Cicha praca","m³/min","4.8","4.8"]
["","","Grzanie","Wysoki","m³/min","11.7","17"]
["","Natężenie przepływu powietrza","Ogrzewanie","Czynnik","m³/min","7.7","10"]
["","","Grzanie","Niski","m³/min","5.6","6"]
["","","","Cicha praca","m³/min","4.7","5.1"]
["Poziom mocy akustycznej","Chłodzenie","","","dBA","60","60"]
["","Ogrzewanie","","","dBA","59","60"]
["Poziom ciśnienia akustycznego","Chłodzenie","","Wysoki","dBA","45","46"]
["","","","Czynnik","dBA","33","32"]
["","","","Niski","dBA","25","24"]
["","","","Cicha praca","dBA","21","20"]
["","Grzanie","","Wysoki","dBA","43","46"]
["","Ogrzewanie","","Czynnik","dBA","31","31"]
["","Grzanie","","Niski","dBA","22","22"]
["","","","Cicha praca","dBA","19","19"]
["Czynnik chłodniczy","GWP","","","","675","675"]
["Połączenia instalacji rurowej","Ciecz","","Śr. zewn.","mm","6.35","6.35"]
["","Gaz","","Śr. zewn.","mm","9.5","9.5"]
["","Spust","","","","18","18"]
["Syst. kontroli","Pilot na podczerwień","","","","ARC466A83","ARC466A83"]
["Standardowe akcesoria","FTXTM30A2V1B","","","","1"]
["","Installation manual","","","","1","1"]
["","Wireless remote control","","","","1","1"]
["","Screw cover","","","","2","2"]
["","AAA dry-cell batteries","","","","2","2"]
["","General safety precautions","","","","1","1"]
["","Operation manual","","","","1","1"]
["","Titanium apatite deodorizing filter","","","","1","1"]
["","Silver particle filter","","","","1","1"]
["","Remote control holder","","","","1","1"]
["","Screw bag","","","","1","1"]
["Zasilanie energią elektryczną","Nazwa","","","","V1","V1"]
["","liczba faz","","","","1~","1~"]
["Zasilanie","Częstotliwość","","","Hz","50","50"]
["","Napięcie","","","V","220-240","220-240"]
["Uwagi","","","","","(1) - Chłodzenie: temp. wewn. 27°CDB, 19,0°CWB; temp. zewn. 35°CDB, 24°CWB; długość równoważna instalacji rurowej: 5 m","(1) - Chłodzenie: temp. wewn. 27°CDB, 19,0°CWB; temp. zewn. 35°CDB, 24°CWB; długość równoważna instalacji rurowej: 5 m"]
["","","","","","(2) - Grzanie: temp. wewn. 20°CDB; temp. zewnętrzna 7°CDB, 6°CWB , równoważna instalacja chłodnicza: 5 m","(2) - Grzanie: temp. wewn. 20°CDB; temp. zewnętrzna 7°CDB, 6°CWB , równoważna instalacja chłodnicza: 5 m"]
["","","","","","(3) - Dane elektryczne, patrz oddzielny rysunek","(3) - Dane elektryczne, patrz oddzielny rysunek"]
["Standardowe akcesoria","FTXTM40A2V1B","","","","","1"]