{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":40,"n_cols":7,"rows_kept":40,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXTM-M"]
[]
[]
[]
[]
["","","","","","FTXTM30M2V1B","FTXTM40M2V1B"]
["Pobór mocy","Chłodzenie","","Nom.","kW","0.032","0.037"]
["","Grzanie","","Nom.","kW","0.037","0.04"]
["Obudowa","Kolor","","","","Biały","Biały"]
["Wymiary","Jednostka","","Wysokość","mm","294","300"]
["","","","Szerokość","mm","811","1040"]
["","","","Głębokość","mm","272","295"]
["Ciężar","Jednostka","","","kg","10","14.5"]
["Wentylator","Przepływ powietrza","Chłodzenie","Wysoki","m³/min","11.7","15.5"]
["","Natężenie przepływu powietrza","Chłodzenie","Czynnik","m³/min","8","9.2"]
["","","","Niski","m³/min","6.3","5.7"]
["","","","Cicha praca","m³/min","5.2","4.6"]
["","","Grzanie","Wysoki","m³/min","12.2","17.7"]
["","Natężenie przepływu powietrza","Ogrzewanie","Czynnik","m³/min","7.5","11"]
["","","Grzanie","Niski","m³/min","5.1","7.5"]
["","","","Cicha praca","m³/min","4.1","6.3"]
["Poziom mocy akustycznej","Chłodzenie","","","dBA","60","60"]
["","Ogrzewanie","","","dBA","61","61"]
["Poziom ciśnienia akustycznego","Chłodzenie","","Wysoki","dBA","45","46"]
["","","","Czynnik","dBA","33","32"]
["","","","Niski","dBA","25","24"]
["","","","Cicha praca","dBA","21","20"]
["","Grzanie","","Wysoki","dBA","45","46"]
["","Ogrzewanie","","Czynnik","dBA","31","31"]
["","Grzanie","","Niski","dBA","22","22"]
["","","","Cicha praca","dBA","19","19"]
["Połączenia instalacji rurowej","Ciecz","","Śr. zewn.","mm","6.35","6.35"]
["","Gaz","","Śr. zewn.","mm","9.5","9.5"]
["","Spust","","","","16 (średnica wewn. łączącego elastycznego przewodu rurowego)","16 (średnica wewn. łączącego elastycznego przewodu rurowego)"]
["Syst. kontroli","Pilot na podczerwień","","","","ARC466A55","ARC466A55"]
["","Pilot przewodowy","","","","BRC944B2, BRC073A1","BRC944B2, BRC073A1"]
["Zasilanie energią elektryczną","Nazwa","","","","V1","V1"]
["","liczba faz","","","","1~","1~"]
["Zasilanie","Częstotliwość","","","Hz","50","50"]
["","Napięcie","","","V","220-240","220-240"]