{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":94,"n_cols":7,"rows_kept":94,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXTM-R"]
[]
[]
[]
[]
["","","","","","FTXTM30R2V1B","FTXTM40R2V1B"]
["Poziom ciśnienia akustycznego","Grzanie","","Wysoki","dBA","45.0"]
["","","","Czynnik","dBA","31.0"]
["","","","Cicha praca","dBA","19.0"]
["","","","Niski","dBA","22.0"]
["","Chłodzenie","","Czynnik","dBA","33.0"]
["","","","Cicha praca","dBA","21.0"]
["","","","Niski","dBA","25.0"]
["","","","Wysoki","dBA","45.0"]
["Standardowe akcesoria","Instrukcja instalacji","","","","1"]
["","Instrukcja obsługi","","","","1"]
["","Pilot bezprzewodowy","","","","1"]
["","Baterie suche typu AAA","","","","2"]
["","Uchwyt do pilota","","","","1"]
["","Płyta montażowa","","","","1"]
["","Śruby mocujące jednostkę wewnętrzną","","","","2"]
["","Filtr z cząsteczkami srebra","","","","1"]
["Control systems","Wired remote control","","","","BRC073A1"]
["","Infrared remote control","","","","ARC466A75"]
["Połączenia instalacji rurowej","Ciecz","","Śr. zewn.","mm","6.35"]
["","Gaz","","Śr. zewn.","mm","9.50"]
["","Spust","","","","18"]
["Power input","Chłodzenie","","Nom.","kW","0.035"]
["","Ogrzewanie","","Nom.","kW","0.039"]
["Sound power level","Chłodzenie","","","dBA","60.0"]
["","Ogrzewanie","","","dBA","61.0"]
["Wymiary","Jednostka","","Szerokość","mm","778"]
["","","","Głębokość","mm","272"]
["","","","Wysokość","mm","295"]
["Casing","Kolor","","","","Biały"]
["Ciężar","Jednostka","","","kg","10.0"]
["Fan","Przepływ powietrza","Grzanie","Wysoki","m³/min","12.5"]
["","","","Niski","m³/min","4.9"]
["","","","Czynnik","m³/min","7.5"]
["","","","Cicha praca","m³/min","4.0"]
["","","Chłodzenie","Niski","m³/min","5.3"]
["","","","Czynnik","m³/min","7.8"]
["","","","Wysoki","m³/min","12.2"]
["","","","Cicha praca","m³/min","4.1"]
["Power supply","liczba faz","","","","1~"]
["","Częstotliwość","","","Hz","50"]
["","Nazwa","","","","V1"]
["","Napięcie","","","V","220-240"]
["Uwagi","","","","","(1) - Chłodzenie: temp. wewn. 27°CDB, 19,0°CWB; temp. zewnętrznej 35°CDB, 24°CWB; długość równoważna instalacji rurowej: 5 m"]
["","","","","","(2) - Grzanie: temp. wewn. 20°CDB; temp. zewnętrzna 7°CDB, 6°CWB , równoważna instalacja chłodnicza: 5 m"]
["","","","","","(3) - Dane elektryczne, patrz oddzielne rysunki"]
["Pobór mocy","Chłodzenie","","Nom.","kW","","0.053"]
["","Grzanie","","Nom.","kW","","0.06"]
["Obudowa","Kolor","","","","","Biały"]
["Wymiary","Jednostka","","Wysokość","mm","","299"]
["","","","Szerokość","mm","","998"]
["","","","Głębokość","mm","","292"]
["Ciężar","Jednostka","","","kg","","14.5"]
["Wentylator","Przepływ powietrza","Chłodzenie","Wysoki","m³/min","","15.4"]
["","Natężenie przepływu powietrza","Chłodzenie","Czynnik","m³/min","","9.5"]
["","","","Niski","m³/min","","5.8"]
["","","","Cicha praca","m³/min","","4.6"]
["","","Grzanie","Wysoki","m³/min","","17.5"]
["","Natężenie przepływu powietrza","Ogrzewanie","Czynnik","m³/min","","10.5"]
["","","Grzanie","Niski","m³/min","","7.1"]
["","","","Cicha praca","m³/min","","5.9"]
["Poziom mocy akustycznej","Chłodzenie","","","dBA","","60"]
["","Ogrzewanie","","","dBA","","61"]
["Poziom ciśnienia akustycznego","Chłodzenie","","Wysoki","dBA","","46"]
["","","","Czynnik","dBA","","32"]
["","","","Niski","dBA","","24"]
["","","","Cicha praca","dBA","","20"]
["","Grzanie","","Wysoki","dBA","","46"]
["","Ogrzewanie","","Czynnik","dBA","","31"]
["","Grzanie","","Niski","dBA","","22"]
["","","","Cicha praca","dBA","","19"]
["Połączenia instalacji rurowej","Ciecz","","Śr. zewn.","mm","","6.35"]
["","Gaz","","Śr. zewn.","mm","","9.5"]
["","Spust","","","","","18"]
["Control systems","Infrared remote control","","","","","ARC466A75"]
["Syst. kontroli","Pilot przewodowy","","","","","BRC073A1"]
["Standardowe akcesoria","Installation manual","","","","","1"]
["","Wireless remote control","","","","","1"]
["","AAA dry-cell batteries","","","","","2"]
["","Operation manual","","","","","1"]
["","Titanium apatite deodorizing filter","","","","","1"]
["","Silver particle filter","","","","","1"]
["","Indoor unit fixing screws","","","","","2"]
["","Mounting plate","","","","","1"]
["","Remote control holder","","","","","1"]
["Zasilanie energią elektryczną","Nazwa","","","","","V1"]
["","liczba faz","","","","","1~"]
["Zasilanie","Częstotliwość","","","Hz","","50"]
["","Napięcie","","","V","","220-240"]