{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":30,"n_cols":6,"rows_kept":30,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXTM-S / RXTM-A"]
[]
[]
[]
[]
["","","","","FTXTM30S2V1B / RXTM30A2V1B","FTXTM40S2V1B / RXTM40A2V1B"]
["Wydajność chłodnicza","Min.","","kW","1.2","1.2"]
["","Nom.","","kW","3","4"]
["","Maks.","","kW","4.6","5.2"]
["Wydajność grzewcza","Min.","","kW","0.8","0.9"]
["","Nom.","","kW","3.2","4"]
["","Maks.","","kW","7.4","8.8"]
["Wydaj. znam.","EER","","","5.13","4.71"]
["","COP","","","5.2","5.51"]
["","Rocz. zużycie ener.","","kWh","292","425"]
["Efektywność nominalna","Dyrektywa na temat oznaczeń zużycia energii (klas energetycznych)","Chłodzenie","","A","A"]
["","","Ogrzewanie","","A","A"]
["Chłodzenie pomieszczeń","Klasa efektywności energetycznej","","","A+++","A+++"]
["","Wydajność","Pdesign","kW","3","4"]
["","SEER","","","8.65","8.93"]
["","Roczne zużycie energii","","kWh/rok","121","157"]
["Ogrzewanie pomieszczeń (przeciętny klimat)","Klasa efektywności energetycznej","","","A+++","A+++"]
["","Wydajność","Pdesign","kW","3","3.8"]
["","SCOP/A","","","5.2","5.5"]
["","Pdh Wydajność grzewcza w temp. -10°","","kW","3","3.8"]
["","Roczne zużycie energii","","kWh/rok","807","967"]
["Uwagi","","","","(1) - Dane elektryczne, patrz oddzielny rysunek","(1) - Dane elektryczne, patrz oddzielny rysunek"]
["","","","","(2) - Patrz oddzielny rysunek zakresu pracy","(2) - Patrz oddzielny rysunek zakresu pracy"]
["","","","","(3) - Nominalne wydajności chłodzenia oparte są na: temp. wewnętrzna: 27°CDB, 19°CWB, temp. zewn.: 35°CDB, równoważna dług. rur: 5 m, różnica poziomów: 0 m.","(3) - Nominalne wydajności chłodzenia oparte są na: temp. wewnętrzna: 27°CDB, 19°CWB, temp. zewn.: 35°CDB, równoważna dług. rur: 5 m, różnica poziomów: 0 m."]
["","","","","(4) - Nominalne wydajności grzewcze oparte są na: temperaturze wewnętrznej: 20°CDB; temperaturze zewnętrznej: 7°CDB, 6°CWB , równorzędnej instalacji chłodniczej: 5 m, różnicy poziomów: 0 m.","(4) - Nominalne wydajności grzewcze oparte są na: temperaturze wewnętrznej: 20°CDB; temperaturze zewnętrznej: 7°CDB, 6°CWB , równorzędnej instalacji chłodniczej: 5 m, różnicy poziomów: 0 m."]