{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":55,"n_cols":7,"rows_kept":55,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXTP-A"]
[]
[]
[]
[]
["","","","","","FTXTP25A5V1B","FTXTP35A5V1B"]
["Pobór mocy","Chłodzenie","","Nom.","kW","0.032","0.032"]
["","Grzanie","","Nom.","kW","0.032","0.032"]
["Obudowa","Kolor","","","","Biały","Biały"]
["Wymiary","Jednostka","","Wysokość","mm","286","286"]
["","","","Szerokość","mm","770","770"]
["","","","Głębokość","mm","225","225"]
["Ciężar","Jednostka","","","kg__","9","9"]
["Wentylator","Przepływ powietrza","Chłodzenie","Wysoki","m³/min","11","11"]
["","Natężenie przepływu powietrza","Chłodzenie","Czynnik","m³/min","7.9","7.9"]
["","","","Niski","m³/min","5","5"]
["","","","Cicha praca","m³/min","3.7","3.7"]
["","","Grzanie","Wysoki","m³/min","10.5","10.5"]
["","Natężenie przepływu powietrza","Ogrzewanie","Czynnik","m³/min","9","9"]
["","","Grzanie","Niski","m³/min","5.5","5.5"]
["","","","Cicha praca","m³/min","4.4","4.4"]
["Poziom mocy akustycznej","Chłodzenie","","","dBA","58","58"]
["","Ogrzewanie","","","dBA","58","58"]
["Poziom ciśnienia akustycznego","Chłodzenie","","Wysoki","dBA","43","43"]
["","","","Czynnik","dBA","35","35"]
["","","","Niski","dBA","26","26"]
["","","","Cicha praca","dBA","21","21"]
["","Grzanie","","Wysoki","dBA","43","43"]
["","Ogrzewanie","","Czynnik","dBA","35","35"]
["","Grzanie","","Niski","dBA","26","26"]
["","","","Cicha praca","dBA","21","21"]
["Czynnik chłodniczy","GWP","","","","675","675"]
["Połączenia instalacji rurowej","Ciecz","","Śr. zewn.","mm","6.35","6.35"]
["","Gaz","","Śr. zewn.","mm","9.5","9.5"]
["","Spust","","","","18","18"]
["Syst. kontroli","Infrared remote control","","","","ARC480A78","ARC480A78"]
["Standardowe akcesoria","FTXTP25A5V1B","","","","1"]
["","Installation manual","","","","1","1"]
["","Wireless remote control","","","","1","1"]
["","Screw cover","","","","2","2"]
["","AAA dry-cell batteries","","","","2","2"]
["","General safety precautions","","","","1","1"]
["","Operation manual","","","","1","1"]
["","Titanium apatite deodorizing filter","","","","1","1"]
["","Silver particle filter","","","","1","1"]
["","Remote control holder","","","","1","1"]
["","Screw bag","","","","1","1"]
["Zasilanie energią elektryczną","Nazwa","","","","V1","V1"]
["","liczba faz","","","","1~","1~"]
["Zasilanie","Częstotliwość","","","Hz","50","50"]
["","Napięcie","","","V","220-240","220-240"]
["Uwagi","","","","","(1) - Chłodzenie: temp. wewn. 27°CDB, 19,0°CWB; temp. zewn. 35°CDB, 24°CWB; długość równoważna instalacji rurowej: 5 m","(1) - Chłodzenie: temp. wewn. 27°CDB, 19,0°CWB; temp. zewn. 35°CDB, 24°CWB; długość równoważna instalacji rurowej: 5 m"]
["","","","","","(2) - Grzanie: temp. wewn. 20°CDB; temp. zewnętrzna 7°CDB, 6°CWB , równoważna instalacja chłodnicza: 5 m","(2) - Grzanie: temp. wewn. 20°CDB; temp. zewnętrzna 7°CDB, 6°CWB , równoważna instalacja chłodnicza: 5 m"]
["","","","","","(3) - Dane elektryczne, patrz oddzielny rysunek","(3) - Dane elektryczne, patrz oddzielny rysunek"]
["Standardowe akcesoria","FTXTP35A5V1B","","","","","1"]