{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":83,"n_cols":7,"rows_kept":83,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXTP-K"]
[]
[]
[]
[]
["","","","","","FTXTP25K3V1B","FTXTP35K3V1B"]
["Poziom ciś. akust.","Grzanie","","Wysoki","dBA","43"]
["","","","Czynnik","dBA","35"]
["","","","Cicha praca","dBA","21"]
["","","","Niski","dBA","26"]
["","Chłodzenie","","Czynnik","dBA","35"]
["","","","Cicha praca","dBA","21"]
["","","","Niski","dBA","26"]
["","","","Wysoki","dBA","43"]
["Standardowe akcesoria","Instrukcja instalacji","","","","1"]
["","Instrukcja obsługi","","","","1"]
["","Pilot bezprzewodowy","","","","1"]
["","Baterie suche typu AAA","","","","2"]
["","Uchwyt do pilota","","","","1"]
["","Płyta montażowa","","","","1"]
["","Tytanowo-apatytowy filtr eliminujący zapachy","","","","2"]
["","Śruby mocujące jednostkę wewnętrzną","","","","2"]
["Control systems","Wired remote control","","","","BRC944B2, BRC073A1"]
["","Infrared remote control","","","","ARC480A11"]
["Piping connections","Ciecz","","Śr. zewn.","mm","6.35"]
["","Gaz","","Śr. zewn.","mm","9.50"]
["","Drain","","","","16 (średnica wewn. łączącego elastycznego przewodu rurowego)"]
["Power input","Chłodzenie","","Nom.","kW","0.030"]
["","Grzanie","","Nom.","kW","0.035"]
["Poziom mocy akustycznej","Chłodzenie","","","dBA","58"]
["","Ogrzewanie","","","dBA","58"]
["Wymiary","Jednostka","","Szerokość","mm","770"]
["","","","Głębokość","mm","225"]
["","","","Wysokość","mm","285"]
["Obudowa","Colour","","","","Biały"]
["Ciężar","Jednostka","","","kg","9.0"]
["Power supply","Phase","","","","1~"]
["","Częstotliwość","","","Hz","50"]
["","Nazwa","","","","V1"]
["","Napięcie","","","V","220-240"]
["Uwagi","","","","","(1) - Dane elektryczne, patrz oddzielny rysunek"]
["Pobór mocy","Chłodzenie","","Nom.","kW","","0.03"]
["","Grzanie","","Nom.","kW","","0.035"]
["Obudowa","Kolor","","","","","Biały"]
["Wymiary","Jednostka","","Wysokość","mm","","285"]
["","","","Szerokość","mm","","770"]
["","","","Głębokość","mm","","225"]
["Ciężar","Jednostka","","","kg","","9"]
["Wentylator","Przepływ powietrza","Chłodzenie","Wysoki","m³/min","","11.4"]
["","Natężenie przepływu powietrza","Chłodzenie","Czynnik","m³/min","","8.2"]
["","","","Niski","m³/min","","5.4"]
["","","","Cicha praca","m³/min","","4.3"]
["","","Grzanie","Wysoki","m³/min","","10.8"]
["","Natężenie przepływu powietrza","Ogrzewanie","Czynnik","m³/min","","7.8"]
["","","Grzanie","Niski","m³/min","","5.8"]
["","","","Cicha praca","m³/min","","4.9"]
["Poziom mocy akustycznej","Chłodzenie","","","dBA","","58"]
["","Ogrzewanie","","","dBA","","58"]
["Poziom ciśnienia akustycznego","Chłodzenie","","Wysoki","dBA","","43"]
["","","","Czynnik","dBA","","35"]
["","","","Niski","dBA","","26"]
["","","","Cicha praca","dBA","","21"]
["","Grzanie","","Wysoki","dBA","","43"]
["","Ogrzewanie","","Czynnik","dBA","","35"]
["","Grzanie","","Niski","dBA","","26"]
["","","","Cicha praca","dBA","","21"]
["Połączenia instalacji rurowej","Ciecz","","Śr. zewn.","mm","","6.35"]
["","Gaz","","Śr. zewn.","mm","","9.5"]
["","Spust","","","","","16 (średnica wewn. łączącego elastycznego przewodu rurowego)"]
["Control systems","Infrared remote control","","","","","ARC480A11"]
["Syst. kontroli","Pilot przewodowy","","","","","BRC944B2, BRC073A1"]
["Standardowe akcesoria","Installation manual","","","","","1"]
["","Wireless remote control","","","","","1"]
["","AAA dry-cell batteries","","","","","2"]
["","Operation manual","","","","","1"]
["","Titanium apatite deodorizing filter","","","","","2"]
["","Indoor unit fixing screws","","","","","2"]
["","Mounting plate","","","","","1"]
["","Remote control holder","","","","","1"]
["Zasilanie energią elektryczną","Nazwa","","","","","V1"]
["","liczba faz","","","","","1~"]
["Zasilanie","Częstotliwość","","","Hz","","50"]
["","Napięcie","","","V","","220-240"]