{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":21,"n_cols":8,"rows_kept":21,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXV-AB"]
[]
[]
[]
[]
["","","","","FTXV25AV1B","FTXV35AV1B","FTXV50AV1B","FTXV60AV1B"]
["Poziom ciśnienia akustycznego","Chłodzenie","Cicha praca","dBA","28","30","35","39"]
["","","Niski","dBA","34","35","40","42"]
["","","Wysoki","dBA","41","42","48","51"]
["","","Nom.","dBA","39","40","43","47"]
["Control systems","Infrared remote control","","","ARC470A21","ARC470A21","ARC470A21","ARC470A21"]
["Połączenia instalacji","Ciecz","Śr. zewn.","mm","6.35","6.35","6.35","6.35"]
["","Gaz","Śr. zewn.","mm","9.52","9.52","12.70","15.9"]
["Sound power level","Chłodzenie","","dBA","50","51","53","57"]
["Wymiary","Jednostka","Szerokość","mm","845","845","940","1,007"]
["","","Głębokość","mm","180","180","200","219"]
["","","Wysokość","mm","275","275","298","315"]
["Ciężar","Jednostka","","kg","9","9","12","14"]
["Power supply","liczba faz","","","1~","1~","1~","1~"]
["","Częstotliwość","","Hz","50","50","50","50"]
["","Napięcie","","V","220-240","220-240","220-240","220-240"]