{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":49,"n_cols":8,"rows_kept":49,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXZ-N"]
[]
[]
[]
[]
["","","","","","FTXZ25NV1B","FTXZ35NV1B","FTXZ50NV1B"]
["Poziom ciśnienia akustycznego","Grzanie","","Wysoki","dBA","39","42","44"]
["","","","Cicha praca","dBA","19","19","24"]
["","","","Niski","dBA","28","29","31"]
["","Chłodzenie","","Cicha praca","dBA","19","19","23"]
["","","","Niski","dBA","26","27","30"]
["","","","Wysoki","dBA","38","42","47"]
["","","","Nom.","dBA","35","36","38"]
["","Chłodzenie","","Nom.","dBA","33","35","38"]
["Standardowe akcesoria","Filtr oczyszczający powietrze oraz fotokatalityczny filtr usuwający nieprzyjemne zapachy","","","","1","1","1"]
["","Pilot bezprzewodowy","","","","1","1","1"]
["","Suche baterie","","","","2","2","2"]
["","Uchwyt do pilota","","","","1","1","1"]
["","Śruby mocujące jednostkę wewnętrzną","","","","3","3","3"]
["","Płyta montażowa","","","","1","1","1"]
["Systemy sterujące","Infrared remote control","","","","ARC477A1","ARC477A1","ARC477A1"]
["Połączenia instalacji rurowej","Ciecz","","Śr. zewn.","mm","6.35","6.35","6.35"]
["","Gaz","","Śr. zewn.","mm","9.5","9.5","9.5"]
["Power input","Chłodzenie","","Nom.","kW","0.030","0.030","0.030"]
["","Grzanie","","Nom.","kW","0.030","0.030","0.030"]
["Sound power level","Chłodzenie","","","dBA","54","57","60"]
["","Ogrzewanie","","","dBA","56","57","59"]
["Wymiary","Jednostka","","Szerokość","mm","798","798","798"]
["","","","Głębokość","mm","372","372","372"]
["","","","Wysokość","mm","295","295","295"]
["Casing","Colour","","","","Biały","Biały","Biały"]
["Ciężar","Jednostka","","","kg__","15","15","15"]
["Wentylator","Przepływ powietrza","Grzanie","Wysoki","m³/min","11.7","13.3","14.4"]
["","","","Niski","m³/min","6.7","6.9","7.7"]
["","","","Cicha praca","m³/min","4.8","4.8","5.9"]
["","","Chłodzenie","Niski","m³/min","5.3","5.6","6.6"]
["","","","Wysoki","m³/min","10.7","12.1","15.0"]
["","","","Cicha praca","m³/min","4.0","4.0","4.6"]
["","","","Nom.","m³/min","8.6","9.2","10.7"]
["","","Chłodzenie","Nom.","m³/min","7.5","8.4","9.2"]
["Power supply","Phase","","","","1~","1~","1~"]
["","Nazwa","","","","V1","V1","V1"]
["","Częstotliwość","","","Hz","50","50","50"]
["","Napięcie","","","V","220-240","220-240","220-240"]
["Uwagi","","","","","(1) - 220 V","(1) - 220 V","(1) - 220 V"]
["","","","","","(2) - 230 V","(2) - 230 V","(2) - 230 V"]
["","","","","","(3) - 240 V","(3) - 240 V","(3) - 240 V"]
["","","","","","(4) - Przód wymiennika ciepła","(4) - Przód wymiennika ciepła","(4) - Przód wymiennika ciepła"]
["","","","","","(5) - Tył wymiennika ciepła","(5) - Tył wymiennika ciepła","(5) - Tył wymiennika ciepła"]