{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":82,"n_cols":11,"rows_kept":82,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FUA-A"]
[]
[]
[]
[]
["","","","","","FUA71AVEB9","FUA100AVEB9","FUA125AVEB9","FUA71AVEB (Archived)","FUA100AVEB (Archived)","FUA125AVEB (Archived)"]
["Poziom ciśnienia akustycznego","Grzanie","","Wysoki","dBA","","","","41","46","47"]
["","","","Czynnik","dBA","","","","38","42","43"]
["","","","Niski","dBA","","","","35","39","40"]
["","Chłodzenie","","Medium","dBA","","","","38","42","43"]
["","","","Niski","dBA","","","","35","39","40"]
["","","","Wysoki","dBA","","","","41","46","47"]
["Standardowe akcesoria","Instrukcja obsługi","","","","","","","1","1","1"]
["","Instrukcja instalacji","","","","","","","1","1","1"]
["","Przewód spustowy","","","","","","","1","1","1"]
["","Rura izolacji cieplnej","","","","","","","3","3","3"]
["","Wiązania","","","","","","","10","10","10"]
["","Opaska zaciskowa przewodu elastycznego","","","","","","","1","1","1"]
["","Materiał uszczelniający","","","","","","","4","4","4"]
["","Płyta mocująca z podkładką","","","","","","","1","1","1"]
["","Złącze spustowe","","","","","","","1","1","1"]
["","włóknina","","","","","","","1","1","1"]
["","Podkładka","","","","","","","8","8","8"]
["","Śruba mocująca dla przewodu spustowego","","","","","","","5","5","5"]
["Syst. kontroli","Wired remote control","","","","","","","BRC1H52W/S/K, BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52","BRC1H52W/S/K, BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52","BRC1H52W/S/K, BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52"]
["Wydajność chłodnicza","Całkowita wydajność","","Nom.","kW","","","","","","12.1"]
["Połączenia instalacji","Ciecz","","Śr. zewn.","mm","","","","9.52","9.52","9.52"]
["","Gaz","","Śr. zewn.","mm","","","","15.9","15.9","15.9"]
["","Spust","","","","","","","VP25 (OD Ø32.0)","VP25 (OD Ø32.0)","VP25 (OD Ø32.0)"]
["Sound power level","Chłodzenie","","","dBA","","","","59","64","65"]
["","Ogrzewanie","","","dBA","","","","59","64"]
["Wymiary","Jednostka","","Szerokość","mm","","","","950","950","950"]
["","","","Głębokość","mm","","","","950","950","950"]
["","","","Wysokość","mm","","","","198","198","198"]
["Obudowa","Materiał","","","","","","","Żywica","Żywica","Żywica"]
["","Kolor","","","","","","","Świeży biały","Świeży biały","Świeży biały"]
["Ciężar","Jednostka","","","kg","","","","25.0","26.0","26"]
["Wentylator","Przepływ powietrza","Grzanie","Wysoki","m³/min","","","","23.0","31.0","32.5"]
["","","","Medium","m³/min","","","","19.5","25.5","26.5"]
["","","","Niski","m³/min","","","","16.0","20.0","20.5"]
["","","Chłodzenie","Niski","m³/min","","","","16.0","20.0","20.5"]
["","","","Medium","m³/min","","","","19.5","25.5","26.5"]
["","","","Wysoki","m³/min","","","","23.0","31.0","32.5"]
["Wysokość spustu","mm","","","","","","","600","600","600"]
["Wydajność grzewcza","Wydajność całkowita","","Nom.","kW","","","","","","13.5"]
["Obudowa","Kolor","","","","Świeży biały","Świeży biały","Świeży biały"]
["","Materiał","","","","Żywica","Żywica","Żywica"]
["Wymiary","Jednostka","","Wysokość","mm","198","198","198"]
["","","","Szerokość","mm","950","950","950"]
["","","","Głębokość","mm","950","950","950"]
["Ciężar","Jednostka","","","kg","25.0","26.0","26.0"]
["Wentylator","Przepływ powietrza","Chłodzenie","Wysoki","m³/min","23.0","31.0","32.5"]
["","Natężenie przepływu powietrza","Chłodzenie","Czynnik","m³/min","19.5","25.5","26.5"]
["","","","Niski","m³/min","16.0","20.0","20.5"]
["","","Grzanie","Wysoki","m³/min","23.0","31.0","32.5"]
["","Natężenie przepływu powietrza","Ogrzewanie","Czynnik","m³/min","19.5","25.5","26.5"]
["","","Grzanie","Niski","m³/min","16.0","20.0","20.5"]
["Poziom mocy akustycznej","Chłodzenie","","","dBA","59","64","65"]
["Poziom ciśnienia akustycznego","Chłodzenie","","Wysoki","dBA","41","46","47"]
["","","","Czynnik","dBA","38","42","43"]
["","","","Niski","dBA","35","39","40"]
["","Grzanie","","Wysoki","dBA","41","46","47"]
["","Ogrzewanie","","Czynnik","dBA","38","42","43"]
["","Grzanie","","Niski","dBA","35","39","40"]
["Połączenia instalacji rurowej","Ciecz","","Śr. zewn.","mm","9.52","9.52","9.52"]
["","Gaz","","Śr. zewn.","mm","15.9","15.9","15.9"]
["","Spust","","","","VP25 (OD Ø32.0)","VP25 (OD Ø32.0)","VP25 (OD Ø32.0)"]
["Wysokość spustu","mm","","","","600","600","600"]
["Standardowe akcesoria","Installation manual","","","","1","1","1"]
["","Thermal insulation tube","","","","3","3","3"]
["","Non woven fabric","","","","1","1","1"]
["","Drain joint","","","","1","1","1"]
["","Hose band","","","","1","1","1"]
["","Operation manual","","","","1","1","1"]
["","Drain hose","","","","1","1","1"]
["","Fixing screw for drain hose","","","","5","5","5"]
["","Sealing material","","","","4","4","4"]
["","Tie-wraps","","","","10","10","10"]
["","Washer","","","","8","8","8"]
["","Washer fixing plate","","","","1","1","1"]
["Wydajność chłodnicza","Całkowita wydajność","","Nom.","kW","","","12.10"]
["Wydajność grzewcza","Wydajność całkowita","","Nom.","kW","","","13.5"]