{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":23,"n_cols":11,"rows_kept":23,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FVQ-C / RZQG-L(8)Y1"]
[]
[]
[]
[]
["","","","","FVQ100CVEB / RZQG71L8Y1B","FVQ71CVEB / RZQG71L8Y1B","FVQ140CVEB / RZQG100L8Y1B","FVQ100CVEB / RZQG100L8Y1B","FVQ140CVEB / RZQG125L8Y1B","FVQ125CVEB / RZQG125L8Y1B","FVQ140CVEB / RZQG140L7Y1B"]
["Wydajność chłodnicza","Nom.","","kW","","6.8","","9.5","","12.0","13.4"]
["Chłodzenie pomieszczeń","SEER","","","6.31","6.23","5.61","5.61","5.61","5.61"]
["","Roczne zużycie energii","","kWh/rok","378","383","593","593","749","748.663"]
["","Wydajność","Pdesign","kW","6.80","6.80","9.50","9.5","12.00","12.00"]
["","Klasa efektywności energetycznej","","","A++","A++","A+","A+","A+","A+"]
["Ogrzewanie pomieszczeń (przeciętny klimat)","Wydajność","Pdesign","kW","6.33","6.33","11.30","11.3","11.30","11.30"]
["","SCOP/A","","","4.05","4.05","4.20","4.2","3.87","3.87"]
["","Klasa efektywności energetycznej","","","A+","A+","A+","A+","A","A"]
["","Roczne zużycie energii","","kWh/rok","2,189","2,189","3,767","3,767","4,088","4,087.855"]
["Efektywność nominalna","Rocz. zużycie ener.","","kWh","","1,010","","1,245","","1,870","2,085"]
["","EER","","","","3.37","","3.81","","3.21","3.21"]
["","COP","","","","3.64","","4.14","","3.70","3.61"]
["","Dyrektywa na temat oznaczeń zużycia energii (klas energetycznych)","Chłodzenie","","","A","","A","","A"]
["","","Ogrzewanie","","","A","","A","","A"]
["Wydajność grzewcza","Nom.","","kW","","7.5","","10.8","","13.5","15.5"]
["Uwagi","","","","","(1) - Roczne zużycie energii jest zgodne z Dyrektywą na temat oznaczeń konsumpcji energii 2002/31/WE","","(1) - Wartości EER/COP według Eurovent 2012, do użytkowania tylko poza Unią Europejską","","(1) - Wartości EER/COP według Eurovent 2012, do użytkowania tylko poza Unią Europejską","(1) - Wartości EER/COP według Eurovent 2012, do użytkowania tylko poza Unią Europejską"]
["","","","","","(2) - Współczynniki SEER i SCOP zgodne z EN 14825","","(2) - Wydaj. znam.: (chłodzenie przy temp. 35°/27° i obciążeniu znam., grzanie przy temp. 7°/20° i obciążeniu znam.)","","(2) - Wydaj. znam.: (chłodzenie przy temp. 35°/27° i obciążeniu znam., grzanie przy temp. 7°/20° i obciążeniu znam.)","(2) - Wydaj. znam.: (chłodzenie przy temp. 35°/27° i obciążeniu znam., grzanie przy temp. 7°/20° i obciążeniu znam.)"]