{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":40,"n_cols":8,"rows_kept":40,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FVQ-C"]
[]
[]
[]
[]
["","","","","FVQ71CVEB","FVQ100CVEB","FVQ125CVEB","FVQ140CVEB"]
["Poziom ciśnienia akustycznego","Grzanie","Wysoki","dBA","43","50","51","53"]
["","","Nom.","dBA","41","47","48","51"]
["","","Niski","dBA","38","44","46","48"]
["","Chłodzenie","Niski","dBA","38","44","46","48"]
["","","Wysoki","dBA","43","50","51","53"]
["","","Nom.","dBA","41","47","48","51"]
["Standardowe akcesoria","Instrukcja obsługi","","","Instrukcja obsługi","Instrukcja obsługi","Instrukcja obsługi","Instrukcja obsługi"]
["","Instrukcja instalacji","","","Instrukcja instalacji","Instrukcja instalacji","Instrukcja instalacji","Instrukcja instalacji"]
["","Uchwyt montażowy","","","Uchwyt montażowy","Uchwyt montażowy","Uchwyt montażowy","Uchwyt montażowy"]
["","Element gumowy zabezpieczający otwór","","","Element gumowy zabezpieczający otwór","Element gumowy zabezpieczający otwór","Element gumowy zabezpieczający otwór","Element gumowy zabezpieczający otwór"]
["","Tuleja","","","Tuleja","Tuleja","Tuleja","Tuleja"]
["","Izolacja mocowania","","","Izolacja mocowania","Izolacja mocowania","Izolacja mocowania","Izolacja mocowania"]
["","Pokrywa","","","Pokrywa","Pokrywa","Pokrywa","Pokrywa"]
["","Zaciski","","","Zaciski","Zaciski","Zaciski","Zaciski"]
["","Śruby","","","Śruby","Śruby","Śruby","Śruby"]
["","Wzór instalacji","","","Wzór instalacji","Wzór instalacji","Wzór instalacji","Wzór instalacji"]
["","Materiał odporny na kondensację","","","Materiał odporny na kondensację","Materiał odporny na kondensację","Materiał odporny na kondensację","Materiał odporny na kondensację"]
["","Okablowanie zdalnego sterownika","","","Okablowanie zdalnego sterownika","Okablowanie zdalnego sterownika","Okablowanie zdalnego sterownika","Okablowanie zdalnego sterownika"]
["Systemy sterujące","Pilot przewodowy","","","BRC1D52, BRC1E52A/B","BRC1D52, BRC1E52A/B","BRC1D52, BRC1E52A/B","BRC1D52, BRC1E52A/B"]
["Połączenia instalacji rurowej","Ciecz","Śr. zewn.","mm","9.52","9.52","9.52","9.52"]
["","Gaz","Śr. zewn.","mm","15.9","15.9","15.9","15.9"]
["","Spust","","","I.D. 20/O.D. 26","I.D. 20/O.D. 26","I.D. 20/O.D. 26","I.D. 20/O.D. 26"]
["Power input","Chłodzenie","Nom.","kW","0.117","0.238","0.238","0.276"]
["","Grzanie","Nom.","kW","0.117","0.238","0.238","0.276"]
["Poziom mocy akustycznej","Chłodzenie","","dBA","55","62","63","65"]
["","Ogrzewanie","","dBA","55","62","63","65"]
["Wymiary","Jednostka","Szerokość","mm","600","600","600","600"]
["","","Głębokość","mm","270","350","350","350"]
["","","Wysokość","mm","1,850","1,850","1,850","1,850"]
["Obudowa","Kolor","","","Świeży biały","Świeży biały","Świeży biały","Świeży biały"]
["Ciężar","Jednostka","","kg","39","47","47","47"]
["Power supply","liczba faz","","","1~","1~","1~","1~"]
["","Częstotliwość","","Hz","50/60","50/60","50/60","50/60"]
["","Napięcie","","V","220-240/220","220-240/220","220-240/220","220-240/220"]