{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":54,"n_cols":8,"rows_kept":54,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FVXM-B"]
[]
[]
[]
[]
["","","","","","FVXM25B2V1B","FVXM35B2V1B","FVXM50B2V1B"]
["Pobór mocy","Chłodzenie","","Nom.","kW","0.02","0.02","0.03"]
["","Grzanie","","Nom.","kW","0.02","0.03","0.03"]
["Obudowa","Kolor","","","","Biały","Biały","Biały"]
["Wymiary","Jednostka","","Wysokość","mm","600","600","600"]
["","","","Szerokość","mm","750","750","750"]
["","","","Głębokość","mm","238","238","238"]
["Ciężar","Jednostka","","","kg","17","17","17"]
["Wentylator","Przepływ powietrza","Chłodzenie","Wysoki","m³/min","8.7","9.2","11.6"]
["","Natężenie przepływu powietrza","Chłodzenie","Czynnik","m³/min","7","7","9"]
["","","","Niski","m³/min","4.9","4.9","6.6"]
["","","","Cicha praca","m³/min","4.1","4.1","5.4"]
["","","Grzanie","Wysoki","m³/min","9.2","9.8","12.8"]
["","Natężenie przepływu powietrza","Ogrzewanie","Czynnik","m³/min","7.2","7.2","10"]
["","","Grzanie","Niski","m³/min","5.6","5.6","8.4"]
["","","","Cicha praca","m³/min","4.1","4.1","5.9"]
["Poziom mocy akustycznej","Chłodzenie","","","dBA","52","53","61"]
["","Ogrzewanie","","","dBA","52","53","62"]
["Poziom ciśnienia akustycznego","Chłodzenie","","Wysoki","dBA","38","39","44"]
["","","","Czynnik","dBA","32","32","38"]
["","","","Niski","dBA","25","25","31"]
["","","","Cicha praca","dBA","20","20","27"]
["","Grzanie","","Wysoki","dBA","38","39","46"]
["","Ogrzewanie","","Czynnik","dBA","32","32","40"]
["","Grzanie","","Niski","dBA","25","25","35"]
["","","","Cicha praca","dBA","19","19","29"]
["Czynnik chłodniczy","GWP","","","","675","675","675"]
["Połączenia instalacji rurowej","Ciecz","","Śr. zewn.","mm","6.4","6.4","6.4"]
["","Gaz","","Śr. zewn.","mm","9.5","9.5","12.7"]
["","Spust","","","","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)"]
["Syst. kontroli","Pilot na podczerwień","","","","ARC466A90","ARC466A90","ARC466A90"]
["","Pilot przewodowy","","","","BRC073A1","BRC073A1","BRC073A1"]
["Standardowe akcesoria","FVXM25B2V1B","","","","1"]
["","Installation manual","","","","1","1","1"]
["","Wireless remote control","","","","1","1","1"]
["","AAA dry-cell batteries","","","","2","2","2"]
["","General safety precautions","","","","1","1","1"]
["","Operation manual","","","","1","1","1"]
["","Titanium apatite deodorizing filter","","","","2","2","2"]
["","Remote control holder","","","","1","1","1"]
["","Screw bag","","","","1","1","1"]
["Zasilanie energią elektryczną","Nazwa","","","","V1","V1","V1"]
["","liczba faz","","","","1~","1~","1~"]
["Zasilanie","Częstotliwość","","","Hz","50","50","50"]
["","Napięcie","","","V","220-240","220-240","220-240"]
["Uwagi","","","","","(1) - Chłodzenie: temp. wewn. 27°CDB, 19,0°CWB; temp. zewn. 35°CDB, 24°CWB; długość równoważna instalacji rurowej: 5 m","(1) - Chłodzenie: temp. wewn. 27°CDB, 19,0°CWB; temp. zewn. 35°CDB, 24°CWB; długość równoważna instalacji rurowej: 5 m","(1) - Chłodzenie: temp. wewn. 27°CDB, 19,0°CWB; temp. zewn. 35°CDB, 24°CWB; długość równoważna instalacji rurowej: 5 m"]
["","","","","","(2) - Grzanie: temp. wewn. 20°CDB; temp. zewnętrzna 7°CDB, 6°CWB , równoważna instalacja chłodnicza: 5 m","(2) - Grzanie: temp. wewn. 20°CDB; temp. zewnętrzna 7°CDB, 6°CWB , równoważna instalacja chłodnicza: 5 m","(2) - Grzanie: temp. wewn. 20°CDB; temp. zewnętrzna 7°CDB, 6°CWB , równoważna instalacja chłodnicza: 5 m"]
["Standardowe akcesoria","FVXM35B2V1B","","","","","1"]
["","FVXM50B2V1B","","","","","","1"]