{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":77,"n_cols":11,"rows_kept":77,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FWXT-ATV3"]
[]
[]
[]
[]
["","","","","","FWXT10ABTV3","FWXT15ABTV3","FWXT20ABTV3","FWXT10AATV3 (Archived)","FWXT15AATV3 (Archived)","FWXT20AATV3 (Archived)"]
["Wymiary","Jednostka","","Szerokość","mm","","","","902","1,100","1,300"]
["","","","Głębokość","mm","","","","128","128","128"]
["","","","Wysokość","mm","","","","335","335","335"]
["Obudowa","Kolor","","","","","","","BIAŁY (RAL 9003)","BIAŁY (RAL 9003)","BIAŁY (RAL 9003)"]
["Ciężar","Jednostka","","","kg","","","","14.0","16.0","19.0"]
["Power supply","liczba faz","","","","","","","1~","1~","1~"]
["","Częstotliwość","","","Hz","","","","50","50","50"]
["","Napięcie","","","V","","","","230","230","230"]
["Wydajność chłodnicza","7/12°C","","Min.","kW","0.49","0.62","0.70"]
["","","","Śred.","kW","0.88","1.08","1.21"]
["","","","Maks.","kW","1.24","1.61","1.94"]
["Jawna wydajność chłodnicza","7/12°C","","Min.","kW","0.37","0.52","0.57"]
["","","","Śred.","kW","0.70","0.86","1.02"]
["","","","Maks.","kW","0.98","1.27","1.52"]
["Wydajność grzewcza","45/40°C","","Min.","kW","0.55","0.79","0.74"]
["","","","Śred.","kW","1.00","1.36","1.55"]
["","","","Maks.","kW","1.50","2.01","2.13"]
["Pobór mocy","Min.","","","kW","0.01","0.01","0.01"]
["","Śred.","","","kW","0.01","0.01","0.01"]
["","Maks.","","","kW","0.02","0.02","0.03"]
["Prędkość wentylatora","Min.","","","obr/min_","680.00","680.00","680.00"]
["","Śred.","","","obr/min_","1100.00","1100.00","1100.00"]
["","Maks.","","","obr/min_","1500.00","1500.00","1500.00"]
["Obudowa","Kolor","","","","BIAŁY (RAL 9003)","BIAŁY (RAL 9003)","BIAŁY (RAL 9003)"]
["","Materiał","","","","blacha cienka","blacha cienka","blacha cienka"]
["Wymiary","Jednostka","","Wysokość","mm","335","335","335"]
["","","","Szerokość","mm","902","1102","1302"]
["","","","Głębokość","mm","128","128","128"]
["","Jednostka zapakowana","","Wysokość","mm","490","490","490"]
["","","","Szerokość","mm","1030","1230","1430"]
["","","","Głębokość","mm","210","210","210"]
["Ciężar","Jednostka","","","kg","14","16","19"]
["","Jednostka zapakowana","","","kg","15","17","20"]
["Opakowanie","Materiał","","","","Karton","Karton","Karton"]
["","Ciężar","","","kg","1","1","1"]
["Wymiennik ciepła","Ilość","","","","1","1","1"]
["","Objętość wew. wężownicy","","","l","0.5","0.61","0.77"]
["","Ładowanie","","Ciśnienie operacyjne","bar","10","10","10"]
["Obwód wody","Średnica połączeń instalacji rurowej","","","in","3/4","3/4","3/4"]
["Obieg wody","Materiał rur","","","","MIEDŹ","MIEDŹ","MIEDŹ"]
["","Ciśnienie","Grzanie","Maks.","bar","10","10","10"]
["Obieg wody - spadek ciśnienia wody","Ogrzewanie","45/40°C","Min.","kPa","5.10","4.81","6.00"]
["","","","Śred.","kPa","12.00","6.30","6.40"]
["","","","Maks.","kPa","16.30","7.20","8.10"]
["","Chłodzenie","7/12°C","Min.","kPa","4.80","4.70","5.50"]
["","","","Śred.","kPa","10.50","5.60","5.40"]
["","","","Maks.","kPa","11.70","5.10","5.30"]
["Obieg wody - natężenie przepływu wody","Ogrzewanie","45/40°C","Min.","kg/h","100.00","140","150.00"]
["","","","Śred.","kg/h","170.00","240","300.00"]
["","","","Maks.","kg/h","260.00","350","420.00"]
["","Chłodzenie","7/12°C","Min.","kg/h","80.00","110","120.00"]
["","","","Śred.","kg/h","150.00","190","210.00"]
["","","","Maks.","kg/h","210.00","280","330.00"]
["Poziom mocy akustycznej","Min.","","","dBA","35","36","37"]
["","Śred.","","","dBA","46","47","48"]
["","Maks.","","","dBA","53.0","54.0","55.0"]
["Zakres pracy","Grzanie","Strona wodna","Min.","°C","30","30","30"]
["","","","Maks.","°C","85","85","85"]
["","Chłodzenie","Strona wodna","Min.","°C","5","5","5"]
["","","","Maks.","°C","18","18","18"]
["","Montaż w pomieszczeniu","Temp. otoczenia","Min.","°CDB","0","0","0"]
["","","","Maks.","°CDB","45","45","45"]
["Syst. kontroli","Pilot na podczerwień","","","","Dla FWXT-ATV3(C)(CL)","Dla FWXT-ATV3(C)(CL)","Dla FWXT-ATV3(C)(CL)"]
["","Wbudowany w jednostkę wewnętrzną","","","","Tak","Tak","Tak"]
["Zasilanie energią elektryczną","liczba faz","","","","1~","1~","1~"]
["Zasilanie","Częstotliwość","","","Hz","50","50","50"]
["","Napięcie","","","V","230","230","230"]
["Pobór mocy elektrycznej","Maks.","","","W","19","20","29"]
["","Tryb gotowości","","","W","3","4","5"]
["Prąd","Maksymalny prąd roboczy","","Grzanie","A","0.16","0.18","0.24"]
["","Maks. prąd roboczy","","Chłodzenie","A","0.16","0.18","0.24"]