{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":35,"n_cols":5,"rows_kept":35,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FXMQ-P7H"]
[]
[]
[]
[]
["","","","","FXMQ50P7VEH"]
["Czynnik chłodniczy","Typ","","","R-410A"]
["Wydajność chłodnicza","Nom.","","kW","5.6 (1)"]
["Połączenia instalacji","Ciecz","Śr. zewn.","mm","6.35"]
["","","Typ","","Połączenie rozszerzające"]
["","Gaz","Śr. zewn.","mm","12.7"]
["","","Typ","","Połączenie rozszerzające"]
["","Spust","","","VP25 (I.D. 25/O.D. 32)"]
["Wymagana przestrzeń międzystropowa >","mm","","","350"]
["Wymiary","Jednostka","Szerokość","mm","1,000"]
["","","Głębokość","mm","700"]
["","","Wysokość","mm","300"]
["Obudowa","Materiał","","","Galwanizowana blacha stalowa"]
["","Kolor","","","Nie powlekana"]
["Ciężar","Jednostka","","kg","35"]
["Wentylator","Spręż dyspozycyjny - 60Hz","Wysoki","Pa","200"]
["Wysokość spustu","mm","","","625"]
["Panel dekoracyjny","Ciężar","","kg","4.5"]
["","Model","","","BYBS71DJW1"]
["","Wymiary","Wysokość","mm","55"]
["","","Głębokość","mm","500"]
["","","Szerokość","mm","1,100"]
["","Kolor","","","Biały (10Y9/0,5)"]
["Wydajność grzewcza","Nom.","","kW","6.3 (2)"]
["Power supply","liczba faz","","","1~"]
["","Częstotliwość","","Hz","50/60"]
["","Nazwa","","","VE"]
["","Napięcie","","V","220-240/220 +/-10%"]
["Uwagi","","","","(1) - Chłodzenie: temp. wewn. 27°CDB, 19,0°CWB; temp. zewn. 35°CDB; długość równoważna instalacji rurowej: 7,5m; różnica poziomów: 0 m"]
["","","","","(2) - Grzanie: temp. wewn. 20°CDB; temp. zewnętrzna 7°CDB, 6°CWB , równoważna instalacja chłodnicza: 7,5 m; różnica poziomów: 0 m"]