{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":22,"n_cols":7,"rows_kept":22,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","HCU-PXB1"]
[]
[]
[]
[]
["","","","","","HCU2040PXB1","HCU4070PXB1"]
["Wydajność chłodnicza","Niskotemperaturowe","","kW","kW","3.03","6.56"]
["Sprężarka","Liczba obrotów","","","obr/min_","4,800","3,600"]
["Ciężar","Jednostka","","","kg","161","300"]
["Fan motor","Moc wy.","","","W","115","230"]
["","Napęd","","","","EC","EC"]
["Wymiennik ciepła","Typ","","","","Miedź/aluminium, standard","Miedź/aluminium, standard"]
["Power input","Niskotemperaturowe","","Nom.","kW","3.79","7.05"]
["COP","Low temperature","","Nom.","","0.80","0.93"]
["Wymiary","Jednostka","","Szerokość","mm","574","773"]
["","","","Głębokość","mm","1,452","1,684"]
["","","","Wysokość","mm","799","1,438"]
["Silnik wentylatora","Wyjście","","","W","115","230"]
["Obudowa","Kolor","","","","Jasny szary - RAL 7035","Jasny szary - RAL 7035"]
["Wentylator","Typ","","","","Osiowy","Osiowy"]
["","Przepływ powietrza","Chłodzenie","Nom.","m³/min","63","126"]
["","Ilość","","","","1","2"]