{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":31,"n_cols":7,"rows_kept":31,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","HXHD-A8"]
[]
[]
[]
[]
["","","","","","HXHD125A8V1B","HXHD200A8Y1B"]
["Obudowa","Kolor","","","","Szary metalik","Szary metalik"]
["","Materiał","","","","Arkusz metalowy z powłoką wstępną","Arkusz metalowy z powłoką wstępną"]
["Wymiary","Jednostka","","Wysokość","mm","705","705"]
["","","","Szerokość","mm","600","600"]
["","","","Głębokość","mm","695","695"]
["Ciężar","Jednostka","","","kg","92","147"]
["Czynnik chłodniczy","Typ","","","","R-134a","R-134a"]
["","Ilość","","","kg","2","2.6"]
["Poziom mocy akustycznej","Nom.","","","dBA","55","60"]
["Poziom ciśnienia akustycznego","Nom.","","","dBA","42, 43","46, 46"]
["Zakres pracy","Grzanie","Strona wodna","Min.","°C","25","25"]
["","","","Maks.","°C","80.0","80.0"]
["Zasilanie energią elektryczną","liczba faz","","","","1~","3~"]
["Zasilanie","Częstotliwość","","","Hz","50","50"]
["","Napięcie","","","V","220-240","380-415"]
["Prąd","zalecane bezpieczniki","","","A","20","16"]
["Uwagi","","","","","(1) - EW 40°C; LW 45°C; Dt 5°C; warunki otoczenia: 7°CDB/6°CWB","(1) - EW 40°C; LW 45°C; Dt 5°C; warunki otoczenia: 7°CDB/6°CWB"]
["","","","","","(2) - Dla wody Dt 5°C","(2) - Dla wody Dt 10°C"]
["","","","","","(3) - Poziomy hałasu zmierzone przy: EW 55°C; LW 65°C","(3) - Poziomy hałasu zmierzone przy: EW 55°C; LW 65°C"]
["","","","","","(4) - Poziomy hałasu zmierzone przy: EW 70°C; LW 80°C","(4) - Poziomy hałasu zmierzone przy: EW 70°C; LW 80°C"]
["","","","","","(5) - Ustawienie do montażu","(5) - Ustawienie do montażu"]
["","","","","","(6) - Zgodnie z EN/IEC 61000-3-11, może się okazać konieczna konsultacja z operatorem sieci dystrybucji, aby upewnić się że sprzęt jest podłączony tylko do zasilania Zsys (impedancja systemu) ≤ Zmax","(6) - Zgodnie z EN/IEC 61000-3-11, może się okazać konieczna konsultacja z operatorem sieci dystrybucji, aby upewnić się że sprzęt jest podłączony tylko do zasilania Zsys (impedancja systemu) ≤ Zmax"]
["","","","","","(7) - Europejskie/międzynarodowa norma techniczne określają wartości graniczne zmian napięcia, wahania napięcia i migotania w publicznych sieciach niskiego napięcia dla urządzeń o prądzie znamionowym  ≤ 75A.","(7) - Europejskie/międzynarodowa norma techniczne określają wartości graniczne zmian napięcia, wahania napięcia i migotania w publicznych sieciach niskiego napięcia dla urządzeń o prądzie znamionowym  ≤ 75A."]
["","","","","","(8) - Zsys: impedancja systemu","(8) - Zsys: impedancja systemu"]
["","","","","","(9) - Moc krótkiego spięcia","(9) - Moc krótkiego spięcia"]