{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":30,"n_cols":6,"rows_kept":30,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","LRNUN-AY1"]
[]
[]
[]
[]
["","","","","","LRNUN5A7Y1"]
["Standardowe akcesoria","Deklaracja zgodności","","","","1"]
["Ciężar","Jednostka","","","kg","173"]
["Czynnik chłodniczy","GWP","","","","1.0"]
["","Dopełnienie","","","kg","3.20"]
["Fan motor","Moc wy.","","","W","350"]
["Wymiennik ciepła","Typ","","","","Wężownica z żebrami krzyżowymi"]
["Wymiary","Jednostka","","Szerokość","mm","635"]
["","","","Głębokość","mm","765"]
["","","","Wysokość","mm","1,680"]
["Obudowa","Kolor","","","","Kość słoniowa"]
["Wentylator","Typ","","","","Wentylator śmigłowy"]
["","Przepływ powietrza","Chłodzenie","Nom.","m³/min","102"]
["","Ilość","","","","1"]
["Power supply","liczba faz","","","","3N~"]
["","Częstotliwość","","","Hz","50"]
["","Napięcie","","","V","380-415"]
["Uwagi","","","","","(1) - LRYEN10A7Y1+LRNUN5A7Y1"]
["","","","","","(2) - Sprężarka 1"]
["","","","","","(3) - Sprężarka 2"]
["","","","","","(4) - Sprężarka 3"]
["","","","","","(5) - Ładunek fabryczny jednostki"]
["","","","","","(6) - Dopuszczono do stosowania tylko K65 Ciśnienie 120 barów jest dopuszczalne w przypadku połączeń orurowania AC."]
["","","","","","(7) - Ciśnienie zaworu bezpieczeństwa jest wskazywane  jako ciśnienie manometru."]
["","","","","","(8) - Dopuszczono do stosowania tylko K65 Ciśnienie 90 barów jest dopuszczalne w przypadku orurowania chłodniczego."]