{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":42,"n_cols":6,"rows_kept":42,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","LRYEQ-AY"]
[]
[]
[]
[]
["","","","","","LRYEQ16A7Y1"]
["Standardowe akcesoria","Instrukcja instalacji","","","","1"]
["","Instrukcja obsługi","","","","1"]
["","Łączniki rurowe","","","","1"]
["","Etykieta czynnika chłodniczego do regulacji gazu F","","","","1"]
["","Etykieta z informacją o ładunku czynnika chłodniczego","","","","1"]
["","Wielojęzyczna etykieta z informacją o fluorowanych gazach cieplarnianych","","","","1"]
["Ciężar","Jednostka","","","kg","370"]
["Czynnik chłodniczy","Charge","","","TCO2Eq","24.0"]
["","GWP","","","","2,087.5"]
["","Ilość","","","kg","11.5"]
["","Typ","","","","R-410A"]
["Fan motor","Moc oddawana","","","W","750"]
["","Napęd","","","","Napęd bezpośredni"]
["Wymiennik ciepła","Typ","","","","Wężownica z żebrami krzyżowymi"]
["Wymiary","Jednostka","","Szerokość","mm","1,240"]
["","","","Głębokość","mm","765"]
["","","","Wysokość","mm","1,680"]
["Obudowa","Colour","","","","Kość słoniowa"]
["Wentylator","Type","","","","Wentylator śmigłowy"]
["","Natężenie przepływu powietrza","Chłodzenie","Nom.","m³/min","230"]
["","Ilość","","","","2"]
["Power supply","liczba faz","","","","3~"]
["","Częstotliwość","","","Hz","50"]
["","Napięcie","","","V","380-415"]
["Uwagi","","","","","(1) - Tryb priorytetowy chłodzenia: temp. wewn. 27°CDB, 19°CWB; temp. zewnętrzna 32°CDB; długość instalacji rurowej: 7,5 m; różnica poziomów: 0 m"]
["","","","","","(2) - Tryb priorytetowy chłodzenia: temp. parowania -10°C; temp. zewnętrzna 32°CDB; Ssanie SH: 10°C"]
["","","","","","(3) - Tryb odzyskiwania ciepła 100%: temp. wewn. 20°CDB; temp. zewnętrzna 7°CDB, 6°CWB; ładunek czynnika chłodniczego 18 kW; długość instalacji rurowej: 7,5 m; różnica poziomów: 0 m"]
["","","","","","(4) - Temperatura nasycenia równa ciśnieniu ssania  (strona chłodzenia): -10°C (w warunkach schładzania); wydajność połączenia klimatyzatora wewnętrznego: 10 HP, kiedy odzyskiwanie ciepła wynosi 100%"]
["","","","","","(5) - Sprężarka 1"]
["","","","","","(6) - Sprężarka 2"]
["","","","","","(7) - Sprężarka 3"]
["","","","","","(8) - Ładunek fabryczny jednostki"]
["","","","","","(9) - Zamontować oddzielacz oleju 5 m od jednostki zewnętrznej"]
["","","","","","(10) - Więcej szczegółów widać na rysunku zakresu pracy"]
["","","","","","(11) - Patrz podręcznik instalacji/obsługi, aby uzyskać więcej szczegółowych informacji"]
["","","","","","(12) - Zawiera fluorowane gazy cieplarniane"]