{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":49,"n_cols":6,"rows_kept":49,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","MC55W"]
[]
[]
[]
[]
["","","","","","MC55WVM"]
["Typ","","","","","Oczyszczacz powietrza"]
["Zastosowanie","","","","","Typ przypodłogowy"]
["Obudowa","Kolor","","","","Biały"]
["Wymiary","Jednostka","","Wysokość","mm","500"]
["","","","Szerokość","mm","270"]
["","","","Głębokość","mm","270"]
["Ciężar","Jednostka","","","kg","6.8"]
["Zastosowanie do pomieszczeń o powierzchni","m²","","","","41 (1), 82 (2)"]
["CADR","m³/h","","","","320"]
["Oczyszczanie powietrza","Pobór mocy","","Turbo","kW","0.037"]
["","","","M","kW","0.015"]
["","","","L","kW","0.010"]
["","","","Cichy","kW","0.008"]
["Poziom ciśnienia akustycznego","Oczyszczanie powietrza","","Turbo","dBA","53"]
["","","","Średni","dBA","39"]
["","","","Niski","dBA","29"]
["","","","Cichy","dBA","19"]
["Wentylator","Przepływ powietrza","Oczyszczanie powietrza","Turbo","m³/h","330"]
["","","","Średni","m³/h","192"]
["","","","Niski","m³/h","120"]
["","","","Cichy","m³/h","66"]
["Metoda pochłaniania kurzu","","","","","Filtr elektrostatyczny HEPA"]
["Deodorizing method","","","","","Technologia Flash streamer + Katalizator usuwający zapachy"]
["Urządzenia bezpieczeństwa","Pozycja","","01","","Safety switch (Operation stops when the Streamer unit cover is open)"]
["Standardowe akcesoria","Zdalny sterownik","","","","1"]
["","Uchwyt do pilota","","","","1"]
["","Filtr elektrostatyczny HEPA","","","","1"]
["","Filtr eliminujący zapachy","","","","1"]
["","Instrukcja obsługi","","","","1"]
["Przewód zasilający","m","","","","1.8"]
["Power supply","liczba faz","","","","1~"]
["","Częstotliwość","","","Hz","50/60"]
["","Napięcie","","","V","220-240/220-230"]
["Prąd roboczy","Oczyszczanie powietrza","","Turbo","A","0.32"]
["","","","Średni","A","0.14"]
["","","","Niski","A","0.10"]
["","","","Cichy","A","0.08"]
["Uwagi","","","","","(1) - Odpowiednia powierzchnia pomieszczenia jest odpowiednia dla pracy jednostki z maksymalną prędkością wentylatora (HH). Odpowiednia powierzchnia pomieszczenia to powierzchnia, w jakiej pewna ilość cząsteczek kurzu zostaje usunięta w ciągu 30 minut. (JEM 1467)"]
["","","","","","(2) - Konwersja z wartości testowych do standardów NRCC zgodnie z  JEM1467."]
["","","","","","(3) - Konwersja z wartości testowych do standardów CADR zgodnie z  JEM1467."]
["","","","","","(4) - Poziomy głośności podczas pracy to średnia wartości zmierzonych w odległości 1 m od przedniej, lewej, prawej i górnej części urządzenia. (Są one równe wartościom w komorze bezechowej.)"]
["","","","","","(5) - Filtr elektrostatyczny HEPA jest zainstalowany w jednostce."]
["","","","","","(6) - Inne funkcje: Aktywna funkcja plazmowania Funkcja automatycznego ponownego uruchomienia"]