{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":38,"n_cols":6,"rows_kept":38,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","MC80Z"]
[]
[]
[]
[]
["","","","","","MC80ZVM"]
["Typ","","","","","Oczyszczacz powietrza"]
["Zastosowanie","","","","","Typ przypodłogowy"]
["Obudowa","Kolor","","","","Front: White, Top/Side: Dark Grey"]
["Wymiary","Jednostka","","Wysokość","mm","630"]
["","","","Szerokość","mm","315"]
["","","","Głębokość","mm","315"]
["Ciężar","Jednostka","","","kg","9.8"]
["Zastosowanie do pomieszczeń o powierzchni","m²","","","","62, 124"]
["CADR","m³/h","","","","480"]
["Oczyszczanie powietrza","Pobór mocy","","Turbo","kW","0.080"]
["","","","M","kW","0.016"]
["","","","L","kW","0.011"]
["","","","Cichy","kW","0.009"]
["Poziom ciśnienia akustycznego","Oczyszczanie powietrza","","Turbo","dBA","55"]
["","","","Średni","dBA","34"]
["","","","Niski","dBA","25"]
["","","","Cichy","dBA","19"]
["Wentylator","Przepływ powietrza","Oczyszczanie powietrza","Turbo","m³/h","480"]
["","","","Średni","m³/h","210"]
["","","","Niski","m³/h","132"]
["","","","Cichy","m³/h","84"]
["Metoda pochłaniania kurzu","","","","","Filtr elektrostatyczny HEPA"]
["Metoda usuwania zapachów","","","","","Technologia TWIN streamer + katalizator usuwający zapachy"]
["Standardowe akcesoria","Operation manual","","","","1"]
["","Electrostatic HEPA filter","","","","1"]
["","Deodorising filter","","","","1"]
["Przewód zasilający","m","","","","2"]
["Zasilanie energią elektryczną","liczba faz","","","","1~"]
["Zasilanie","Częstotliwość","","","Hz","50/60"]
["","Napięcie","","","V","220-240/220-230"]
["Uwagi","","","","","(1) - Obszar pokrycia jest odpowiedni dla pracy jednostki z maksymalną prędkością wentylatora (HH). Obszar pokrycia to powierzchnia, w jakiej pewna ilość cząsteczek kurzu zostaje usunięta w ciągu 30 minut."]
["","","","","","(2) - Konwersja z wartości testowych do standardów NRCC zgodnie z  JEM1467."]