{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":63,"n_cols":6,"rows_kept":63,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","MCK55W"]
[]
[]
[]
[]
["","","","","","MCK55WVM"]
["Typ","","","","","Oczyszczacz powietrza z funkcją nawilżania"]
["Zastosowanie","","","","","Typ przypodłogowy"]
["Obudowa","Kolor","","","","Biały"]
["Wymiary","Jednostka","","Wysokość","mm","700"]
["","","","Szerokość","mm","270"]
["","","","Głębokość","mm","270"]
["Ciężar","Jednostka","","","kg","9.5"]
["Zastosowanie do pomieszczeń o powierzchni","m²","","","","41 (1), 82 (2)"]
["CADR","m³/h","","","","320"]
["Oczyszczanie powietrza","Pobór mocy","","Turbo","kW","0.056"]
["","","","M","kW","0.017"]
["","","","L","kW","0.010"]
["","","","Cichy","kW","0.007"]
["Nawilżanie","Pobór mocy","","Turbo","kW","0.058"]
["","","","M","kW","0.019"]
["","","","L","kW","0.014"]
["","","","Cichy","kW","0.011"]
["","Pojemność zbiornika wody","","","l","2.7"]
["Poziom ciśnienia akustycznego","Oczyszczanie powietrza","","Turbo","dBA","53.0"]
["","","","Średni","dBA","39.0"]
["","","","Niski","dBA","29.0"]
["","","","Cichy","dBA","19.0"]
["","Nawilżanie","","Turbo","dBA","53.0"]
["","","","Średni","dBA","39.0"]
["","","","Niski","dBA","33.0"]
["","","","Cichy","dBA","25.0"]
["Wentylator","Przepływ powietrza","Oczyszczanie powietrza","Turbo","m³/h","330"]
["","","","Średni","m³/h","192"]
["","","","Niski","m³/h","120"]
["","","","Cichy","m³/h","54"]
["","","Nawilżanie","Turbo","m³/h","330"]
["","","","Średni","m³/h","192"]
["","","","Niski","m³/h","144"]
["","","","Cichy","m³/h","102"]
["Metoda pochłaniania kurzu","","","","","Filtr elektrostatyczny HEPA"]
["Metoda usuwania zapachów","","","","","Technologia Flash streamer + Katalizator usuwający zapachy"]
["Standardowe akcesoria","Operation manual","","","","1"]
["","Electrostatic HEPA filter","","","","1"]
["","Deodorising filter","","","","1"]
["","Caster","","","","4"]
["","Humidifying filter","","","","2"]
["","Remote control holder","","","","1"]
["","Remote control lid","","","","1"]
["Przewód zasilający","Przewód zasilający","","","","1.8"]
["Zasilanie energią elektryczną","liczba faz","","","","1~"]
["Zasilanie","Zasilanie-=-Częstotliwość","","Częstotliwość","","50/60"]
["","Zasilanie-=-Napięcie","","Napięcie","","220-240/220-230"]
["Prąd roboczy","Oczyszczanie powietrza","Prąd roboczy-=-Oczyszczanie powietrza-=-Turbo","Turbo","","0.50"]
["","","Prąd roboczy-=-Oczyszczanie powietrza-=-Średni","Średni","","0.19"]
["","","Prąd roboczy-=-Oczyszczanie powietrza-=-Niski","Niski","","0.12"]
["","","Prąd roboczy-=-Oczyszczanie powietrza-=-Cichy","Cichy","","0.09"]
["","Nawilżanie","Prąd roboczy-=-Nawilżanie-=-Turbo","Turbo","","0.50"]
["","","Prąd roboczy-=-Nawilżanie-=-Średni","Średni","","0.20"]
["","","Prąd roboczy-=-Nawilżanie-=-Niski","Niski","","0.15"]
["","","Prąd roboczy-=-Nawilżanie-=-Cichy","Cichy","","0.13"]
["Uwagi","","","","","(1) - Odpowiednia powierzchnia pomieszczenia jest odpowiednia dla pracy jednostki z maksymalną prędkością wentylatora (HH). Odpowiednia powierzchnia pomieszczenia to powierzchnia, w jakiej pewna ilość cząsteczek kurzu zostaje usunięta w ciągu 30 minut. (JEM 1467)"]
["","","","","","(2) - Konwersja z wartości testowych do standardów NRCC zgodnie z  JEM1467."]