{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":59,"n_cols":6,"rows_kept":59,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","MCK70ZW"]
[]
[]
[]
[]
["","","","","","MCK70ZVM-W"]
["Typ","","","","","Oczyszczacz powietrza z funkcją nawilżania"]
["Zastosowanie","","","","","Typ przypodłogowy"]
["Obudowa","Colour","","","","White (9.9YR/9.4/0.2)"]
["Wymiary","Jednostka","","Wysokość","mm","760"]
["","","","Szerokość","mm","315"]
["","","","Głębokość","mm","315"]
["Ciężar","Jednostka","","","kg","12.5"]
["Zastosowanie do pomieszczeń o powierzchni","m²","","","","48 (1), 96 (2)"]
["CADR","m³/h","","","","375"]
["Oczyszczanie powietrza","Pobór mocy","","Turbo","kW","0.082"]
["","","","M","kW","0.020"]
["","","","L","kW","0.011"]
["","","","Cichy","kW","0.010"]
["Nawilżanie","Pobór mocy","","Turbo","kW","0.084"]
["","","","M","kW","0.023"]
["","","","L","kW","0.012"]
["","","","Cichy","kW","0.010"]
["","Pojemność zbiornika wody","","","l","3.4"]
["Poziom ciśnienia akustycznego","Oczyszczanie powietrza","","Turbo","dBA","54"]
["","","","Średni","dBA","37"]
["","","","Niski","dBA","27"]
["","","","Cichy","dBA","18"]
["","Nawilżanie","","Turbo","dBA","54"]
["","","","Średni","dBA","37"]
["","","","Niski","dBA","27"]
["","","","Cichy","dBA","18"]
["Wentylator","Przepływ powietrza","Oczyszczanie powietrza","Turbo","m³/h","420"]
["","","","Średni","m³/h","210"]
["","","","Niski","m³/h","132"]
["","","","Cichy","m³/h","84"]
["","","Nawilżanie","Turbo","m³/h","420"]
["","","","Średni","m³/h","210"]
["","","","Niski","m³/h","132"]
["","","","Cichy","m³/h","84"]
["Metoda pochłaniania kurzu","","","","","Filtr elektrostatyczny HEPA"]
["Deodorizing method","","","","","Technologia Flash streamer + Katalizator usuwający zapachy"]
["Standardowe akcesoria","Filtr elektrostatyczny HEPA","","","","1"]
["","Filtr nawilżający","","","","2"]
["","Filtr eliminujący zapachy","","","","1"]
["","Instrukcja obsługi i instalacji","","","","1"]
["","Kółko samonastawne","","","","4"]
["Przewód zasilający","m","","","","2"]
["Power supply","liczba faz","","","","1~"]
["","Częstotliwość","","","Hz","50/60"]
["","Napięcie","","","V","220-240/220-230"]
["Uwagi","","","","","(1) - Obszar pokrycia jest odpowiedni dla pracy jednostki z maksymalną prędkością wentylatora (HH). Obszar pokrycia to powierzchnia, w jakiej pewna ilość cząsteczek kurzu zostaje usunięta w ciągu 30 minut."]
["","","","","","(2) - Konwersja z wartości testowych do standardów NRCC zgodnie z  JEM1467."]
["","","","","","(3) - Konwersja z wartości testowych do standardów CADR zgodnie z  JEM1467."]
["","","","","","(4) - Wartość nawilżania zmienia się zgodnie z temperaturą i poziomem wilgotności w pomieszczeniu i na zewnątrz. Warunki pomiaru: 20°temperatura 20°C, poziom wilgotności."]
["","","","","","(5) - Poziomy głośności podczas pracy to średnia wartości zmierzonych w odległości 1 m od przedniej, lewej, prawej i górnej części urządzenia. (Są one równe wartościom w komorze bezechowej.)"]
["","","","","","(6) - Filtr elektrostatyczny HEPA i filtry nawilżające są zainstalowane w jednostce."]
["","","","","","(7) - Wymagania zgodnie z JEM1467."]
["","","","","","(8) - Wyświetla się „HI”, gdy stężenie PM2.5 przekracza 99 µg/m3."]