{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":31,"n_cols":21,"rows_kept":31,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RDV"]
[]
[]
[]
[]
["","","","","","RDV103EA12S3A","RDV103EA12S3B","RDV103EA12S7A","RDV103EA12S7B","RDV105EA12S3A","RDV105EA12S3B","RDV105EA12S7A","RDV105EA12S7B","RDV206EA12S3A","RDV206EA12S3B","RDV206EA12S7A","RDV206EA12S7B","RDV207EA12S3A","RDV207EA12S3B","RDV207EA12S7A","RDV207EA12S7B"]
["Wydajność chłodnicza","Średnia temp.","R-134a","Nom","kW","0.593","","0.593","","0.912","","0.912","","1.336","","1.336","","1.935","","1.935"]
["Wydajność grzewcza","R-134a","","Nom.","kW","","0.7","","0.9","","1.05","","0.9","","1.4","","1.6","","1.75","","1.6"]
["Obudowa","Kolor","","Skraplacz","","fioletowy","fioletowy","fioletowy","fioletowy","fioletowy","fioletowy","fioletowy","fioletowy","fioletowy","fioletowy","fioletowy","fioletowy","fioletowy","fioletowy","fioletowy","fioletowy"]
["Wymiary","Skraplacz","","Szerokość","mm","682","","682","","682","","682","","882","","882","","882","","882"]
["","","","Głębokość","mm","337","","337","","337","","337","","427","","427","","427","","427"]
["","Parownik","","Wysokość","mm","","570","","215","","570","","215","","570","","215","","570","","215"]
["","","","Szerokość","mm","","375","","669","","375","","669","","595","","1089","","595","","1089"]
["","","","Głębokość","mm","","210","","490","","210","","490","","210","","490","","210","","490"]
["Sprężarka","Ilość","","","","1","","1","","1","","1","","1","","1","","1","","1"]
["","Typ","","","","Sprężarka parowa","","Sprężarka parowa","","Sprężarka parowa","","Sprężarka parowa","","Sprężarka parowa","","Sprężarka parowa","","Sprężarka parowa","","Sprężarka parowa"]
["","Model","","","","AE4430Y-FZ1A","","AE4430Y-FZ1A/CSIR","","NEU6212Z/CSI","","NEU6212Z/CSIR","","CAJ4476Y/F/CSIR","","CAJ4476Y/F/CSIR","","CAJ4511Y/F","","CAJ4511Y/F"]
["","Metoda uruchomienia_","","","","Bezpośredni","","Bezpośredni","","Bezpośredni","","Bezpośredni","","Bezpośredni","","Bezpośredni","","Bezpośredni","","Bezpośredni"]
["Skraplacz","Przepływ powietrza","","","m³/h","600","","600","","1200","","1200","","600","","600","","1100","","1100"]
["Parownik","Zasięg strumienia powietrza","","","m","4","","4","","4","","4","","4","","4","","4","","4"]
["Zakres pracy","Temp. w komorze chłodn.","","Min.","°C","10","","10","","10","","10","","10","","10","","10","","10"]
["","","","Maks.","°C","20","","20","","20","","20","","20","","20","","20","","20"]
["","Temp. otoczenia","","Min.","°C","20","","20","","20","","20","","20","","20","","20","","20"]
["","","","Maks.","°C","40","","40","","40","","40","","40","","40","","40","","40"]
["Czynnik chłodniczy","Typ","","","","R-134a","","R-134a","","R-134a","","R-134a","","R-134a","","R-134a","","R-134a","","R-134a"]
["","GWP","","","","1430","","1430","","1430","","1430","","1430","","1430","","1430","","1430"]
["Standard. odbieralnik cieczy","l","","","","1.6","","1.6","","2.5","","2.5","","1.6","","1.6","","2.5","","2.5"]
["Poziom ciśnienia akustycznego","Nom.","","","dBA","35","","35","","35","","35","","43","","43","","43","","43"]
["Zasilanie","Napięcie","","","V","220-230","","220-230","","220-230","","220-230","","220-230","","220-230","","220-230","","220-230"]
["Zasilanie energią elektryczną","liczba faz","","","","1~","","1~","","1~","","1~","","1~","","1~","","1~","","1~"]
["Zasilanie","Częstotliwość","","","Hz","50","","50","","50","","50","","50","","50","","50","","50"]