{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":41,"n_cols":8,"rows_kept":41,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RXA-A8"]
[]
[]
[]
[]
["","","","","","RXA20A5V1B8","RXA25A5V1B8","RXA35A5V1B8"]
["Wymiary","Jednostka","","Wysokość","mm","550","550","550"]
["","","","Szerokość","mm","840","840","840"]
["","","","Głębokość","mm","350","350","350"]
["Ciężar","Jednostka","","","kg","32","32","32"]
["Sprężarka","Typ","","","","Sprężarka typu \"swing\" uszczelniona hermetycznie","Sprężarka typu \"swing\" uszczelniona hermetycznie","Sprężarka typu \"swing\" uszczelniona hermetycznie"]
["Zakres pracy","Chłodzenie","Temp. otoczenia","Min.","°CDB","-10","-10","-10"]
["","","","Maks.","°CDB","46","46","46"]
["","Grzanie","Temp. otoczenia","Min.","°CWB","-15","-15","-15"]
["","","","Maks.","°CWB","18","18","18"]
["Poziom ciśnienia akustycznego","Chłodzenie","","Nom.","dBA","46.0","46.0","49.0"]
["","Grzanie","","Nom.","dBA","47.0","47.0","49.0"]
["Czynnik chłodniczy","Typ","","","","R-32","R-32","R-32"]
["","Ilość","","","kg","0.76","0.76","0.76"]
["","Ilość","","","tCO2Eq","0.52","0.52","0.52"]
["","GWP","","","","675.0","675.0","675.0"]
["Połączenia instalacji","Długość instalacji rurowej","Maks.","OU - IU","m","20","20","20"]
["","Dodatkowy ładunek czynnika chłodniczego","","","kg/m","0,02 (dla długości instalacji rurowej przekraczającej 10 m)","0,02 (dla długości instalacji rurowej przekraczającej 10 m)","0,02 (dla długości instalacji rurowej przekraczającej 10 m)"]
["","Różnica poziomów","IU - OU","Maks.","m","15.0","15.0","15.0"]
["Standardowe akcesoria","Installation manual","","","","1"]
["","Refrigerant charge label","","","","1"]
["","Multilingual fluorinated greenhouse gases labels","","","","1"]
["","General safety precautions","","","","1"]
["","Drain plug","","","","1"]
["Zakres efektywności energetycznej","","","","","A+++ ~ D","A+++ ~ D","A+++ ~ D"]
["Zasilanie energią elektryczną","liczba faz","","","","1~","1~","1~"]
["Zasilanie","Częstotliwość","","","Hz","50","50","50"]
["","Napięcie","","","V","220-240","220-240","220-240"]
["Uwagi","","","","","(1) - Zawiera fluorowane gazy cieplarniane","(1) - Zawiera fluorowane gazy cieplarniane","(1) - Zawiera fluorowane gazy cieplarniane"]
["","","","","","(2) - Patrz oddzielny rysunek zakresu pracy","(2) - Patrz oddzielny rysunek zakresu pracy","(2) - Patrz oddzielny rysunek zakresu pracy"]
["","","","","","(3) - Dane elektryczne, patrz oddzielny rysunek","(3) - Dane elektryczne, patrz oddzielny rysunek","(3) - Dane elektryczne, patrz oddzielny rysunek"]
["Standardowe akcesoria","Instrukcja instalacji","","","","","1","1"]
["","Etykieta z informacją o ładunku czynnika chłodniczego","","","","","1","1"]
["","Wielojęzyczna etykieta z informacją o fluorowanych gazach cieplarnianych","","","","","1","1"]
["","Ogólne zalecenia dotyczące bezpieczeństwa","","","","","1","1"]
["","Korek spustowy","","","","","1","1"]