{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":31,"n_cols":16,"rows_kept":31,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RXB-C"]
[]
[]
[]
[]
["","","","","","RXB20C2V1B","RXB20C5V1B","RXB20C5V1B9","RXB25C2V1B","RXB25C5V1B","RXB25C5V1B9","RXB35C2V1B","RXB35C5V1B","RXB35C5V1B9","RXB50CV1B","RXB60CV1B"]
["Wymiary","Jednostka","","Wysokość","mm","550","550","550","550","550","550","550","550","550","753","753"]
["","","","Szerokość","mm","658","658","658","658","658","658","658","658","658","855","855"]
["","","","Głębokość","mm","275","275","275","275","275","275","275","275","275","328","328"]
["Ciężar","Jednostka","","","kg","28","28","28","28","28","28","30","30","30","44","44"]
["Sprężarka","Typ","","","","Sprężarka typu \"swing\" uszczelniona hermetycznie","Sprężarka typu \"swing\" uszczelniona hermetycznie","Sprężarka typu \"swing\" uszczelniona hermetycznie","Sprężarka typu \"swing\" uszczelniona hermetycznie","Sprężarka typu \"swing\" uszczelniona hermetycznie","Sprężarka typu \"swing\" uszczelniona hermetycznie","Sprężarka typu \"swing\" uszczelniona hermetycznie","Sprężarka typu \"swing\" uszczelniona hermetycznie","Sprężarka typu \"swing\" uszczelniona hermetycznie","Hermetyczny, typ „swing”","Hermetyczny, typ „swing”"]
["Zakres pracy","Chłodzenie","Temp. otoczenia","Min.","°CDB","-10","-10","-10","-10","-10","-10","-10","-10","-10","-10","-10"]
["","","","Maks.","°CDB","46","46","46","46","46","46","46","46","46","46","46"]
["","Grzanie","Temp. otoczenia","Min.","°CWB","-15","-15","-15","-15","-15","-15","-15","-15","-15","-15","-15"]
["","","","Maks.","°CWB","18","18","18","18","18","18","18","18","18","18","18"]
["Poziom ciśnienia akustycznego","Chłodzenie","","Wysoki","dBA","46","46","46","46","46","46","48","48","48"]
["","","","Nom.","dBA","","","","","","","","","","51","51"]
["","Grzanie","","Wysoki","dBA","47","47","47","47","47","47","48","48","48"]
["","","","Nom.","dBA","","","","","","","","","","51","51"]
["Czynnik chłodniczy","Typ","","","","R-410A","R-410A","R-410A","R-410A","R-410A","R-410A","R-410A","R-410A","R-410A","R-410A","R-410A"]
["","Ilość","","","kg","0.74","0.74","0.74","0.74","0.74","0.74","1.0","1.0","1.0","1.45","1.45"]
["","Ilość","","","tCO2Eq","1.5","1.5","1.5","1.5","1.5","1.5","2.1","2.1","2.1","3.0","3.0"]
["","GWP","","","","2087.5","2087.5","2087.5","2087.5","2087.5","2087.5","2087.5","2087.5","2087.5","2087.5","2087.5"]
["Połączenia instalacji","Długość instalacji rurowej","Maks.","OU - IU","m","","","","","","","","","","30","30"]
["Standardowe akcesoria","Installation manual","","","","1","1","1","1","1","1","1","1","1"]
["","Refrigerant charge label","","","","1","1","1","1","1","1","1","1","1"]
["","Multilingual fluorinated greenhouse gases labels","","","","1","1","1","1","1","1","1","1","1"]
["","Drain plug (only heat pump models)","","","","1","1","1","1","1","1","1","1","1"]
["Zasilanie energią elektryczną","liczba faz","","","","1~","1~","1~","1~","1~","1~","1~","1~","1~","1~","1~"]
["Zasilanie","Częstotliwość","","","Hz","50","50","50","50","50","50","50","50","50","50","50"]
["","Napięcie","","","V","220-240","220-240","220-240","220-240","220-240","220-240","220-240","220-240","220-240","220-240","220-240"]