{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":35,"n_cols":10,"rows_kept":35,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RXF-F"]
[]
[]
[]
[]
["","","","","","RXF20F5V1B","RXF25F5V1B","RXF35F5V1B","RXF42F5V1B","RXF50F5V1B"]
["Wymiary","Jednostka","","Wysokość","mm","556","556","556","556","610"]
["","","","Szerokość","mm","740","740","740","740","923"]
["","","","Głębokość","mm","343","343","343","343","367"]
["Ciężar","Jednostka","","","kg","24.0","24.0","24.0","28.0","40.0"]
["Sprężarka","Typ","","","","Sprężarka typu \"swing\" uszczelniona hermetycznie","Sprężarka typu \"swing\" uszczelniona hermetycznie","Sprężarka typu \"swing\" uszczelniona hermetycznie","Sprężarka typu \"swing\" uszczelniona hermetycznie","Sprężarka typu \"swing\" uszczelniona hermetycznie"]
["Zakres pracy","Chłodzenie","Temp. otoczenia","Min.","°CDB","-10","-10","-10","-10","-10"]
["","","","Maks.","°CDB","48","48","48","48","48"]
["","Grzanie","Temp. otoczenia","Min.","°CWB","-15","-15","-15","-15","-15"]
["","","","Maks.","°CWB","18","18","18","18","18"]
["Poziom ciśnienia akustycznego","Chłodzenie","","Wysoki","dBA","46.0","46.0","48.0","48.0","48.0"]
["","Grzanie","","Wysoki","dBA","47.0","47.0","48.0","48.0","49.0"]
["Czynnik chłodniczy","Typ","","","","R-32","R-32","R-32","R-32","R-32"]
["","Ilość","","","kg","0.420","0.420","0.500","0.750","0.800"]
["","Ilość","","","tCO2Eq","0.280","0.280","0.340","0.510","0.540"]
["","GWP","","","","675.0","675.0","675.0","675.0","675.0"]
["Połączenia instalacji","Długość instalacji rurowej","Maks.","OU - IU","m","20","20","20","20","30"]
["","Dodatkowy ładunek czynnika chłodniczego","","","kg/m","002 (dla długości instalacji rurowej przekraczającej 10 m)","002 (dla długości instalacji rurowej przekraczającej 10 m)","002 (dla długości instalacji rurowej przekraczającej 10 m)","002 (dla długości instalacji rurowej przekraczającej 10 m)","002 (dla długości instalacji rurowej przekraczającej 10 m)"]
["","Różnica poziomów","IU - OU","Maks.","m","12.0","12.0","12.0","12.0","20.0"]
["Standardowe akcesoria","Installation manual","","","","1","1","1","1"]
["","Refrigerant charge label","","","","1","1","1","1"]
["","Multilingual fluorinated greenhouse gases labels","","","","1","1","1","1"]
["","General safety precautions","","","","1","1","1","1"]
["","Drain plug","","","","1","1","1","1"]
["Zasilanie energią elektryczną","liczba faz","","","","1~","1~","1~","1~","1~"]
["Zasilanie","Częstotliwość","","","Hz","50","50","50","50","50"]
["","Napięcie","","","V","220-240","220-240","220-240","220-240","220-240"]
["Uwagi","","","","","(1) - Zawiera fluorowane gazy cieplarniane","(1) - Zawiera fluorowane gazy cieplarniane","(1) - Zawiera fluorowane gazy cieplarniane","(1) - Zawiera fluorowane gazy cieplarniane","(1) - Zawiera fluorowane gazy cieplarniane"]
["","","","","","(2) - Dane elektryczne, patrz oddzielny rysunek","(2) - Dane elektryczne, patrz oddzielny rysunek","(2) - Dane elektryczne, patrz oddzielny rysunek","(2) - Dane elektryczne, patrz oddzielny rysunek","(2) - Dane elektryczne, patrz oddzielny rysunek"]
["","","","","","(3) - Patrz oddzielny rysunek zakresu pracy","(3) - Patrz oddzielny rysunek zakresu pracy","(3) - Patrz oddzielny rysunek zakresu pracy","(3) - Patrz oddzielny rysunek zakresu pracy","(3) - Patrz oddzielny rysunek zakresu pracy"]