{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":38,"n_cols":10,"rows_kept":38,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RXL-K"]
[]
[]
[]
[]
["","","","","","RXL20K3V1B","RXL25K3V1B","RXL35K2V1B","RXL42K2V1B","RXL50K2V1B"]
["Wentylator","Natężenie przepływu powietrza","Chłodzenie","Bardzo niska","m³/min","","","30.1","30.6","48.9"]
["","","Ogrzewanie","Bardzo niska","m³/min","","","25.6","27.2","43.1"]
["","","","Bardzo niska","cfm","","","1063","1080","1727"]
["","","Ogrzewanie","Bardzo niska","cfm","","","904","960","1522"]
["Wymiary","Jednostka","","Wysokość","mm","550","550","550","550","735"]
["","","","Szerokość","mm","765","765","765","765","825"]
["","","","Głębokość","mm","285","285","285","285","300"]
["Ciężar","Jednostka","","","kg","34","34","34","39","47"]
["Silnik wentylatora","Prędkość","Chłodzenie","Bardzo niska","obr/min","780","780","780","790","670"]
["","","Ogrzewanie","Bardzo niska","obr/min","740","740","740","780","670"]
["Sprężarka","Type","","","","Sprężarka typu \"swing\" uszczelniona hermetycznie","Sprężarka typu \"swing\" uszczelniona hermetycznie","Sprężarka typu \"swing\" uszczelniona hermetycznie","Sprężarka typu \"swing\" uszczelniona hermetycznie","Sprężarka typu \"swing\" uszczelniona hermetycznie"]
["Zakres pracy","Chłodzenie","Temp. otoczenia","Min.","°CDB","-10","-10","-10","-10","-10"]
["","","","Maks.","°CDB","46","46","46","46","46"]
["","Grzanie","Temp. otoczenia","Min.","°CWB","-25","-25","-25","-25","-25"]
["","","","Maks.","°CWB","18","18","18","18","18"]
["Poziom ciśnienia akustycznego","Chłodzenie","","Wysoki","dBA","46","46","48","48","48"]
["","Grzanie","","Wysoki","dBA","47","47","48","48","48"]
["Czynnik chłodniczy","Typ","","","","R-410A","R-410A","R-410A","R-410A","R-410A"]
["","Ilość","","","kg","1.0","1.05","1.2","1.3","1.7"]
["","Ilość","","","tCO2Eq","2.1","2.2","2.5","2.7","3.5"]
["","GWP","","","","2087.5","2087.5","2087.5","2087.5","2087.5"]
["Połączenia instalacji","Długość instalacji rurowej","Maks.","OU - IU","m","20","20","20","20","30"]
["","Dodatkowy ładunek czynnika chłodniczego","","","kg/m","0,02 (dla długości instalacji rurowej przekraczającej 10 m)","0,02 (dla długości instalacji rurowej przekraczającej 10 m)","0,02 (dla długości instalacji rurowej przekraczającej 10 m)","0,02 (dla długości instalacji rurowej przekraczającej 10 m)","0,02 (dla długości instalacji rurowej przekraczającej 10 m)"]
["","Różnica poziomów","IU - OU","Maks.","m","15","15","15","15","20"]
["Standardowe akcesoria","Installation manual","","","","1","1","1","1","1"]
["","Drain plug","","","","1"]
["Zasilanie energią elektryczną","liczba faz","","","","1~","1~","1~","1~","1~"]
["Zasilanie","Częstotliwość","","","Hz","50","50","50","50","50"]
["","Napięcie","","","V","220-240","220-240","220-230-240","220-230-240","220-230-240"]
["Uwagi","","","","","(1) - 220 V","(1) - 220 V","(1) - 220 V","(1) - 220 V","(1) - 220 V"]
["","","","","","(2) - 230 V","(2) - 230 V","(2) - 230 V","(2) - 230 V","(2) - 230 V"]
["","","","","","(3) - 240 V","(3) - 240 V","(3) - 240 V","(3) - 240 V","(3) - 240 V"]