{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":39,"n_cols":12,"rows_kept":39,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RXM-A"]
[]
[]
[]
[]
["","","","","","RXM20A5V1B","RXM25A5V1B","RXM35A5V1B","RXM42A5V1B","RXM50A5V1B","RXM60A5V1B","RXM71A5V1B"]
["Wymiary","Jednostka","","Wysokość","mm","610","610","610","610","734","734","734"]
["","","","Szerokość","mm","923","923","923","923","954","954","954"]
["","","","Głębokość","mm","367","367","367","367","401","401","401"]
["Ciężar","Jednostka","","","kg","36","36","36","40","49","49","55"]
["Silnik wentylatora","Prędkość","Chłodzenie","Bardzo niska","obr/min_","600","600","600","600","500"]
["Sprężarka","Typ","","","","Sprężarka typu \"swing\" uszczelniona hermetycznie","Sprężarka typu \"swing\" uszczelniona hermetycznie","Sprężarka typu \"swing\" uszczelniona hermetycznie","Sprężarka typu \"swing\" uszczelniona hermetycznie","Sprężarka typu \"swing\" uszczelniona hermetycznie","Sprężarka typu \"swing\" uszczelniona hermetycznie","Sprężarka typu \"swing\" uszczelniona hermetycznie"]
["Zakres pracy","Chłodzenie","Temp. otoczenia","Min.","°CDB","-10","-10","-10","-10","-10","-10","-10"]
["","","","Maks.","°CDB","50","50","50","50","50 (1)","50","46"]
["","Grzanie","Temp. otoczenia","Min.","°CWB","-21","-21","-21","-21","-21 (1)","-21","-15"]
["","","","Maks.","°CWB","18","18","18","18","18","18","18"]
["Poziom ciśnienia akustycznego","Chłodzenie","","Nom.","dBA","46","46","47","48","48","48","47"]
["","Grzanie","","Nom.","dBA","47","47","49","49","49","49","48"]
["Czynnik chłodniczy","Typ","","","","R-32","R-32","R-32","R-32","R-32","R-32","R-32"]
["","Ilość","","","kg","0.95","0.95","0.95","0.95","1.10","1.15","1.15"]
["","Ilość","","","tCO2Eq","0.65","0.65","0.65","0.65","0.75","0.78","0.78"]
["","GWP","","","","675","675","675","675","675","675","675"]
["Połączenia instalacji","Długość instalacji rurowej","Maks.","OU - IU","m","20","20","20","30","30","30","30"]
["","Dodatkowy ładunek czynnika chłodniczego","","","kg/m","0,02 (dla długości instalacji rurowej przekraczającej 10 m)","0,02 (dla długości instalacji rurowej przekraczającej 10 m)","0,02 (dla długości instalacji rurowej przekraczającej 10 m)","0,02 (dla długości instalacji rurowej przekraczającej 10 m)","0,02 (dla długości instalacji rurowej przekraczającej 10 m)","0,02 (dla długości instalacji rurowej przekraczającej 10 m)","0,02 (dla długości instalacji rurowej przekraczającej 10 m)"]
["","Różnica poziomów","IU - OU","Maks.","m","15","15","15","20","20","20","20"]
["Zasilanie energią elektryczną","liczba faz","","","","1~","1~","1~","1~","1~","1~","1~"]
["Zasilanie","Częstotliwość","","","Hz","50","50","50","50","50","50","50"]
["","Napięcie","","","V","220-240","220-240","220-240","220-240","220-240","220-240","220-240"]
["Standardowe akcesoria","Installation manual","","","","1","1","1","1","1","1","1"]
["","Drain joint","","","","1","1","1","1","1"]
["","Refrigerant charge label","","","","1","1","1","1","1","1","1"]
["","Multilingual fluorinated greenhouse gases labels","","","","1","1","1","1","1","1","1"]
["","General safety precautions","","","","1","1","1","1","1"]
["","LOT10 Energy Label","","","","1","1","1","1","1"]
["","Drain cap","","","","3","3","3","3","1","3","3"]
["Uwagi","","","","","","","","","(1) - Patrz oddzielny rysunek zakresu pracy","(1) - Patrz oddzielny rysunek zakresu pracy","(1) - Patrz oddzielny rysunek zakresu pracy"]
["","","","","","","","","","(2) - Dane elektryczne, patrz oddzielny rysunek","(2) - Dane elektryczne, patrz oddzielny rysunek","(2) - Dane elektryczne, patrz oddzielny rysunek"]
["","","","","","","","","","(3) - Zawiera fluorowane gazy cieplarniane","(3) - Zawiera fluorowane gazy cieplarniane","(3) - Zawiera fluorowane gazy cieplarniane"]
["Standardowe akcesoria","Drain plug","","","","","","","","","1","1"]